For 1990-2009 cars

### Removal Procedure

1. Remove the front floor console left side panel. Refer to Console Trim Plate Replacement.
2. Disconnect the park brake warning lamp switch electrical connector (1).
3. Remove the park brake warning lamp switch to park brake lever assembly retaining screw (3).
4. Remove the park brake warning lamp switch (2) from the park brake lever assembly (4).

### Installation Procedure

1. Connect the park brake warning lamp switch electrical connector (1).
2. Install the park brake warning lamp switch (2) to the park brake lever assembly (4).

Notice: Refer to Fastener Notice in the Preface section.

3. Install the park brake warning lamp switch to park brake lever assembly retaining screw (3).

Tighten
Tighten the bolt to 2 Nm (18 lb in).

4. Install the front floor console left side panel. Refer to Console Trim Plate Replacement.