For 1990-2009 cars

### Removal Procedure

1. Remove the air intake duct. Refer to Air Cleaner Assembly Replacement.
2. Remove the accessory drive belt. Refer to Drive Belt Replacement - Accessory.
3. Remove the air conditioning (A/C) drive belt. Refer to Air Conditioning Compressor Belt Replacement.
4. Remove the A/C drive belt tensioner to A/C compressor bracket retaining bolt (1).
5. Remove the A/C drive belt tensioner (2).

### Installation Procedure

1. Install the A/C drive belt tensioner (2).

Notice: Refer to Fastener Notice in the Preface section.

2. Tighten the A/C drive belt tensioner to A/C compressor bracket retaining bolt (1).

Tighten
Tighten the bolt to 22 N·m (16 lb ft).

3. Install the air conditioning (A/C) drive belt. Refer to Air Conditioning Compressor Belt Replacement.
4. Install the accessory drive belt. Refer to Drive Belt Replacement - Accessory.
5. Install the air intake duct. Refer to Air Cleaner Assembly Replacement.