For 1990-2009 cars

### Removal Procedure

Important: If the IPC is being replaced due to mechanical damage only, store the data on Tech 2 so the new IPC can be relearned using the stored info on the Tech 2.

1. Remove the knee Bolster. Refer to Knee Bolster Replacement .
2. Remove the upper steering wheel cover. Refer to Steering Column Trim Covers Replacement .
3. Remove the instrument cluster trim panel. Refer to Instrument Cluster Trim Panel Replacement .
4. Lower the steering column.
5. Remove the instrument cluster (1) to I/P trim pad retaining screws (2).
6. Carefully remove the instrument cluster (1) from the instrument panel trim pad.
7. Disconnect the instrument cluster (1) electrical connector (2).

Important: When removing the instrument cluster, take care not scratch or damage the instrument cluster screen.

8. Remove the instrument cluster (1).

### Installation Procedure

1. Connect the electrical connector (2) to the Instrument cluster (1).

Important: When installing the instrument cluster, make sure the anti-rattle foam (1) is between the I/P trim pad and instrument cluster.

2. Install the instrument cluster.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the instrument cluster (1) retaining screws (2).

Tighten
Tighten the screws (2) to 2 N·m (18 lb in).

4. Install the instrument panel (I/P) trim panel. Refer to Instrument Cluster Trim Panel Replacement .
5. Install the steering wheel upper trim cover. Refer to Steering Column Trim Covers Replacement .
6. Install the knee bolster. Refer to Knee Bolster Replacement .
7. Re-programme the instrument cluster. Refer to Instrument Cluster Programming and Setup .