For 1990-2009 cars

### Removal Procedure

1. Remove the cargo liner. Refer to Cargo Box Liner Replacement .
2. Remove the rear body rail end cover to body retaining screws (1).

Important: Lift the rear of the rear body rail end cover and apply pressure to point (2).

3. Remove the rear body rail end cover (1) from the vehicle.

### Installation Procedure

Important: Guide the front of the rear body rail end cover into position and lower the rear of the body rail end cover into place, applying pressure to point (2).

1. Install the rear body rail end cover (1) to the vehicle.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the rear body rail end cover to body retaining screws (1).

Tighten
Tighten the screws to 6 N·m (53 lb in).

3. Install the cargo liner. Refer to Cargo Box Liner Replacement .