For 1990-2009 cars

### Removal Procedure

1. Remove the right side camshaft position actuators. Refer to Camshaft Position Actuator Replacement - Bank 1 (Right Side) Exhaust and Camshaft Position Actuator Replacement - Bank 1 (Right Side) Intake.
2. Remove the right side camshafts. Refer to Camshaft Removal - Right Side.

### Installation Procedure

1. Install the right side camshafts. Refer to Camshaft Installation - Right Side.
2. Install the right side camshaft position actuators. Refer to Camshaft Position Actuator Replacement - Bank 1 (Right Side) Exhaust and Camshaft Position Actuator Replacement - Bank 1 (Right Side) Intake.