For 1990-2009 cars

Important: Due to the clipping design of the passenger air bag (PAB) module it is extremely difficult to remove from the plastic cradle which is vibration welded to the underside of the Instrument Panel (IP) pad and the metal clips of the PAB would most likely be bent in removing from a pad assembly. This may result in the air bag being deployed incorrectly in an accident should it be re-used with the new IP pad assembly. If replacing the PAB for any reason you must also replace the IP pad assembly.

Refer to Instrument Panel Upper Trim Pad Replacement.