For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Intake Hose Clamp | 7 N·m | 62 lb in
A/C Bracket Bolt | 58 N·m | 43 lb ft
A/C Compressor Belt Idler Pulley Attaching Bolt | 50 N·m | 37 lb ft
A/C Compressor Belt Tensioner Attaching Bolts | 22 N·m | 16 lb ft
A/C Compressor Line - to - Condenser Bolt | 16 N·m | 12 lb ft
Automatic Transmission Cooler Pipe Clamp To A/C Bracket Retaining Bolt | 22 N·m | 16 lb ft
Camshaft Position (CMP) Sensor Bolt | 12 N·m | 106 lb in
Camshaft Retainer Bolts - Hex Head Bolts | 25 N·m | 18 lb ft
Camshaft Retainer Bolts - TORX® Head Bolts | 15 N·m | 11 lb ft
Camshaft Sprocket Bolt - First Pass | 75 N·m | 55 lb ft
Camshaft Sprocket Bolt - Final Pass | 50 degrees
Connecting Rod Bolts - First Pass | 20 N·m | 15 lb ft
Connecting Rod Bolts - Final Pass | 85 degrees
Coolant Air Bleed Pipe and Cover Bolts | 12 N·m | 106 lb in
Coolant Temperature Sensor | 20 N·m | 15 lb ft
Crankshaft Balancer Bolt - Installation Pass to Ensure the Balancer is Completely Installed | 330 N·m | 240 lb ft
Crankshaft Balancer Bolt - First Pass - Install a NEW Bolt After the Installation Pass and Tighten as Described in the First and Final Passes | 50 N·m | 37 lb ft
Crankshaft Balancer Bolt - Final Pass | 140 degrees
Crankshaft Bearing Cap M10 Bolts - First Pass in Sequence | 20 N·m | 15 lb ft
Crankshaft Bearing Cap M10 Bolts - Final Pass in Sequence | 80 degrees
Crankshaft Bearing Cap M10 Studs - First Pass in Sequence | 20 N·m | 15 lb ft
Crankshaft Bearing Cap M10 Studs - Final Pass in Sequence | 51 degrees
Crankshaft Bearing Cap M8 Bolts | 25 N·m | 18 lb ft
Crankshaft Oil Deflector Nuts | 25 N·m | 18 lb ft
Crankshaft Position (CKP) Sensor Bolt | 25 N·m | 18 lb ft
Crankshaft Rear Oil Seal Housing Bolts | 30 N·m | 22 lb ft
Cylinder Head M8 Bolts - in Sequence | 30 N·m | 22 lb ft
Cylinder Head M11 Bolts - First Pass in Sequence | 30 N·m | 22 lb ft
Cylinder Head M11 Bolts - Second Pass in Sequence | 90 degrees
Cylinder Head M11 Bolts - Final Pass in Sequence | 70 degrees
Cylinder Head Coolant Plug | 20 N·m | 15 lb ft
Engine Block Coolant Drain Hole Plug | 60 N·m | 44 lb ft
Engine Block Oil Gallery Plug | 60 N·m | 44 lb ft
Evaporative Emission (EVAP) Canister Purge Solenoid Valve Bracket Bolt | 50 N·m | 37 lb ft
Exhaust Manifold Bolts - First Pass | 15 N·m | 11 lb ft
Exhaust Manifold Bolts - Final Pass | 20 N·m | 15 lb ft
Exhaust Manifold Heat Shield Bolts | 10 N·m | 89 lb in
Flywheel Bolts - First Pass | 20 N·m | 15 lb ft
Flywheel Bolts - Second Pass | 50 N·m | 37 lb ft
Flywheel Bolts - Final Pass | 100 N·m | 74 lb ft
Front Cover Bolts | 25 N·m | 18 lb ft
Fuel Injection Fuel Rail Bolts | 10 N·m | 89 lb in
Ignition Coil Bracket - to - Valve Rocker Arm Cover Studs | 12 N·m | 106 lb in
Ignition Coil - to - Bracket Bolts | 10 N·m | 89 lb in
Intake Manifold Bolts - First Pass in Sequence | 5 N·m | 44 lb in
Intake Manifold Bolts - Final Pass in Sequence | 10 N·m | 89 lb in
J 41798 M8 Bolt | 25 N·m | 18 lb ft
J 41798 M10 Bolts | 50 N·m | 37 lb ft
Knock Sensor Bolts | 25 N·m | 18 lb ft
Oil Filter | 30 N·m | 22 lb ft
Oil Filter Fitting | 55 N·m | 40 lb ft
Oil Level Indicator Tube Bolt | 25 N·m | 18 lb ft
Oil Level Sensor | 20 N·m | 15 lb ft
Oil Pan Baffle Bolts | 12 N·m | 106 lb in
Oil Pan Closeout Cover Bolt | 12 N·m | 106 lb in
Oil Pan Drain Plug | 25 N·m | 18 lb ft
Oil Pan M6 Bolts - Oil Pan - to - Rear Oil Seal Housing | 12 N·m | 106 lb in
Oil Pan M8 Bolts - Oil Pan - to - Engine Block and Oil Pan - to - Front Cover | 25 N·m | 18 lb ft
Oil Pressure Sensor | 35 N·m | 26 lb ft
Oil Pump Cover Bolts | 12 N·m | 106 lb in
Oil Pump Relief Valve Plug | 14 N·m | 106 lb in
Oil Pump Screen Nuts | 25 N·m | 18 lb ft
Oil Pump Screen - to - Oil Pump Bolt | 12 N·m | 106 lb in
Oil Pump - to - Engine Block Bolts | 25 N·m | 18 lb ft
Spark Plugs | 15 N·m | 11 lb ft
Throttle Body Bolts | 10 N·m | 89 lb in
Timing Chain Tensioner Bolts | 25 N·m | 18 lb ft
Valley Cover Bolts | 25 N·m | 18 lb ft
Valve Lifter Guide Bolts | 10 N·m | 89 lb in
Valve Rocker Arm Bolts | 30 N·m | 22 lb ft
Valve Rocker Arm Cover Bolts | 12 N·m | 106 lb in
Water Inlet Housing Bolts | 15 N·m | 11 lb ft
Water Pump Bolts - First Pass | 15 N·m | 11 lb ft
Water Pump Bolts - Final Pass | 30 N·m | 22 lb ft