For 1990-2009 cars

### Removal Procedure

1. Remove five retaining clips (1) securing the upper air cleaner body.
2. Remove upper air cleaner body and air cleaner filter assembly.
3. Remove the air cleaner element from the air cleaner assembly.

Discard the air cleaner element.

### Installation Procedure

1. Install a NEW air cleaner element to the lower air cleaner body.
2. Reassemble the air cleaner element into the upper air cleaner body and place the upper air cleaner body onto the lower air cleaner body.
3. Reinstall the five retaining clips (1) securing the upper air cleaner body to the lower air cleaner body.