For 1990-2009 cars

## Electronic Navigation Antenna Replacement RHD

### Removal Procedure

1. Remove the windshield demister grille. Refer to Defroster Grille Replacement in Instrument Panel, Gages, and Console.
2. Remove the instrument panel (I/P) outer trim cover. Refer to Instrument Panel Outer Trim Cover Replacement in Instrument Panel, Gages, and Console.
3. Grasp the I/P insulation panel assembly (1) and carefully pull downward to disengage the retaining clips.
4. Remove the courtesy lamp socket (2) from the I/P insulation panel assembly (1) by rotating counter-clockwise.
5. Disconnect the navigation interface module (NIM) electrical connector (3).
6. Remove the I/P insulation panel assembly (1).
7. Remove the I/P compartment lower retaining screws (1).
8. Open the I/P compartment door (2).
9. Remove the I/P compartment retaining screw covers (1) from the I/P compartment (2)
10. Remove the I/P compartment upper retaining screws (1).
11. Detach the I/P compartment (2) from the I/P.
12. Disconnect the I/P compartment electrical connector (1).
13. Rotate the navigation module aerial connector lock (1) clockwise and disconnect the navigation module aerial connector (2).
14. Detach the GPS antenna cable retaining clips (2) from the I/P.

Important: The GPS antenna (1) is secured in position with double sided tape.

15. Detach the GPS antenna (1) from the I/P.
16. Pull the GPS antenna cable through the hole (3) in the I/P and remove the GPS antenna (1).

### Installation Procedure

Important: The GPS antenna (1) is secured in position with double sided tape.

1. Install the GPS antenna (1) to the I/P.
2. Feed the GPS antenna cable through the hole (3) in the I/P.
3. Install the GPS antenna cable retaining clips (2) to the I/P.
4. Connect the navigation module aerial connector (2) and rotate the navigation module aerial connector lock (1) counter-clockwise.
5. Connect the I/P compartment electrical connector (1).
6. Install the I/P compartment (2) to the I/P.

Notice: Refer to Fastener Notice in the Preface section.

7. Install the I/P compartment upper retaining screws (1).

Tighten
Tighten the screws to 2 N·m (18 lb in).

8. Install the I/P compartment retaining screw covers (1) into the I/P compartment (2).
9. Close the I/P compartment door (2).
10. Install the I/P compartment lower retaining screws (1).

Tighten
Tighten the screws to 2 N·m (18 lb in).

11. Install the courtesy lamp socket (2) to the I/P insulation panel assembly (1) by rotating clockwise.
12. Connect the NIM electrical connector (3).
13. Install the I/P insulation panel assembly (1) to the I/P by engaging the retaining clips.
14. Make sure all the clips are located correctly.
15. Install the I/P outer trim cover. Refer to Instrument Panel Outer Trim Cover Replacement in Instrument Panel, Gages, and Console.
16. Install the windshield demister grille. Refer to Defroster Grille Replacement in Instrument Panel, Gages, and Console.