For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to General Repair Instructions in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the transmission oil pan. Refer to Automatic Transmission Fluid, Fluid Pan and/or Filter Replacement .
3. Disconnect the vehicle wire harness electrical connector from the transmission electrical connector passage sleeve. Refer to Automatic Transmission Inline 16-Way Connector Description .

1 | Electrical Connector Slide Lock Tip Pull down on the slide lock to remove the sleeve. Push up on the slide lock after sleeve installation.
2 | Electrical Connector Passage Sleeve Tip Use the DT 47715 DT 47715 and J 42183 J 42183 to remove and install the electrical connector passage sleeve.
3 | NEW O-Ring Seals (Qty: 2)
4 | NEW Lip Seal