For 1990-2009 cars

### Removal Procedure

1. Remove the air intake duct. Refer to Air Cleaner Assembly Replacement.
2. Using a suitable tool, rotate the drive belt tensioner (1) clockwise to relieve the tension on the accessory drive belt (2).
3. Remove the accessory drive belt (2).
4. Slowly release tension on the drive belt tensioner (1).
5. Clean and inspect the drive belt surfaces of all the pulleys.

### Installation Procedure

1. Route the accessory drive belt (2) around all the pulleys except the water pump pulley (3).
2. Using a suitable tool, rotate the drive belt tensioner (1) clockwise.
3. Install the accessory drive belt under the water pump pulley (3).
4. Slowly release the drive belt tensioner (1).
5. Install the air intake duct. Refer to Air Cleaner Assembly Replacement.
6. Inspect the accessory drive belt (2) for correct alignment.