For 1990-2009 cars

### Removal Procedure

Caution: Refer to Safety Glasses Caution in the Preface section.

1. Remove the knee bolster. Refer to Knee Bolster Replacement .
2. Remove the floor air outlet duct to instrument panel (I/P) retaining screws (1).
3. Remove the floor air outlet duct (3) from the I/P (2).

### Installation Procedure

1. Install the floor air outlet duct (3) to the instrument panel (I/P) (2).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the floor air outlet duct to I/P retaining screws (1)

Tighten
Tighten the screws to 2 N·m(18 lb in).

3. Install the knee bolster. Refer to Knee Bolster Replacement .