For 1990-2009 cars

The scan tool data lists contain all the instrument panel, gages, and console related parameters that are available on the scan tool. The parameters in the list are arranged in alphabetical order. The data list column indicates the location of the parameter within the scan tool menu selections.

Use the scan tool data lists as directed by a diagnostic table or in order to supplement the diagnostic procedures. Begin all of the diagnostic procedures with the Diagnostic System Check - Vehicle.

Use the scan tool data lists only after the following is determined:

• | There is no published DTC procedure nor published symptom procedure for the customer concern.

• | The DTC or symptom procedure indicated by the diagnostic system check does not resolve the customer concern.

The typical data values are obtained from a correctly operating vehicle under the conditions specified in the first row of the scan tool data list table. Comparison of the parameter values from the suspect vehicle with the typical data values may reveal the source of the customer concern.

Parameter | Operating Conditions | Expected Value | Definition
--- | --- | --- | ---
Ignition is ON, engine OFF, and vehicle is stationary
ABS Telltail | Systems check or fault with the system | On | This parameter displays On, which will command the telltail lamp on the instrument cluster to illuminate when doing a systems check or a fault is logged.
Systems are normal | Off
Alternator Telltail | Fault with the system | On | This parameter displays On, which will command the telltail lamp on the instrument cluster to illuminate when there is a fault with the system.
Systems are normal | Off
Backup System Power Mode | Back up power system activated | Enabled | This parameter displays the status of the backup system power mode.
Back up power system deactivated | Disabled
Battery Voltage | -- | 12 Volts | The scan tool displays 0-14 Volts. The scan tool displays approximately 12 Volts when the ignition is on
Brake Fluid Level Switch | Low brake fluid level | On | This parameter displays On, which will command the telltail lamp on the instrument cluster to illuminate when there is a fault with the system.
Normal brake fluid level | Off
Brake System Telltail | Systems check or fault with the system | On | This parameter displays On, which will command the telltail lamp on the instrument cluster to illuminate when doing a systems check or a fault is logged.
Systems are normal | Off
Current Trip Display | -- | Km | This parameter displays the total distance travelled so far.
Distance To Arrival | -- | Km | This parameter displays the remaining distance till arrival, based off the user's selection.
Door Open Telltail | Door open or ajar | On | This parameter displays On, which will command the telltail lamp on the instrument cluster to illuminate when a door is open or not closed correctly.
Door closed correctly | Off
Drivers Side Seat Belt Telltail | Seat belt not being worn | On | This parameter displays On, which will command the telltail lamp on the instrument cluster to illuminate when doing a systems check or a fault is logged.
Seat belt being worn | Off
Engine Coolant Temperature | -- | [ordm ] C | This parameter displays the current temperature of the coolant in the vehicle in degrees.
Engine Speed | -- | RPM | This parameter displays the speed of the crankshaft as calculated by the control module based on inputs from the crankshaft position (CKP) sensor. The scan tool will display the engine speed in revolutions per minute (RPM).
Fr. Fog Light Telltail | Front fog lamps activated | On | This parameter displays On, which will command the telltail lamp on the instrument cluster to illuminate when turned on.
Front fog lamps deactivated | Off
Fuel Used A | -- | Litres | This parameter displays the total litres of fuel used since the trip computer was reset.
Fuel Used B | -- | Litres | This parameter displays the total litres of fuel used since the trip computer was reset.
High Beam Telltail | High beam activated | On | This parameter displays On, which will command the telltail lamp on the instrument cluster to illuminate when turned on.
High beam deactivated | Off
Ignition Switch | Ignition is in OFF position | Off | This parameter displays the current status of the ignition switch.
Ignition is in ACC position | Off
Ignition is in RUN position | On
Ignition is in CRANK position | On
Left Scroll Switch | -- | Counts | This parameter displays the position of the left scroll switch.
Odometer | -- | Km | This parameter displays the odometer reading which calculates the distance travelled based on information from the ECM.
Phone | Phone activated | On | This parameter displays the commanded state of a connected mobile phone.
Phone deactivated | Off
Rear Fog Light Telltail | Rear fog lights activated | On | This parameter displays On, which will command the telltail lamp on the instrument cluster to illuminate when turned on.
Rear fog lights deactivated | Off
Remaining Fuel | -- | %/ L | This parameter displays the remaining fuel as either a percentage or in litres.
Right Scroll Switch | -- | Counts | This parameter displays the position of the right scroll switch.
Shift Up Indicator | Shift up indicator activated | On | This parameter displays the status of the shift up light.
Shift up indicated deactivated | Off
SRS Air Bag Telltail | Systems check or fault with the system | On | This parameter displays On, which will command the telltail lamp on the instrument cluster to illuminate when doing a systems check or a fault is logged.
Systems are normal | Off
Steering Wheel Switch | Left scroll pressed | Menu Enter | This parameter displays the position of the steering wheel switch.
Left scroll in idle position | Off
System Power Mode | Ignition is in OFF position | Off | This parameter displays the system power mode which is dependant on ignition position.
Ignition is in ACC position | ACC
Ignition is in RUN position | Run
Ignition is in CRANK position | Crank
Time To Arrival | -- | day(s) | This parameter displays the total days remaining till arrival.
Time To Arrival | -- | 00:00:00 (hh:mm:ss) | This parameter displays the time to arrival at a programmed destination.
Tyre Pressure Monitoring Telltail | Systems check or fault with the system | On | This parameter displays On, which will command the telltail lamp on the Instrument Cluster to illuminate when doing a systems check or a fault is logged.
System is normal | Off
Trip A Distance | -- | Km | This parameter displays the total kilometers travelled since last reset.
Trip A Time | -- | day(s) | This parameter will display the total days remaining till arrival.
Trip A Time | -- | 00:00:00 (hh:mm:ss) | This parameter will display the engine running time during this ignition cycle.
Trip B Distance | -- | Km | This parameter displays the total kilometres travelled since last reset.
Trip B Time | -- | day(s) | This parameter displays the total days remaining till arrival.
Trip B Time | -- | 00:00:00 (hh:mm:ss) | This parameter will display the engine running time during this ignition cycle.
Turn Left Signal Telltail | Turn left signal activated | On | This parameter displays On, which will command the telltail lamp on the instrument cluster to illuminate when the turn signal switch is activated.
Turn left signal deactivated | Off
Turn Right Signal Telltail | Turn right signal activated | On | This parameter displays On, which will command the telltail lamp on the instrument cluster to illuminate when the turn signal switch is activated.
Turn left signal deactivated | Off
Vehicle Speed | -- | Km/h | This parameter indicates the vehicle speed calculated by the control module based on an input from the vehicle speed sensor (VSS). The scan tool will display a high value at higher vehicle speeds, and a low value at lower vehicle speeds.
Washer Level Switch | Low washer level | On | This parameter displays the position of the washer level switch.
Normal washer level | Off