For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Clean the surrounding area of the oil pressure test plug.
3. Remove the oil pressure test plug.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the oil pressure test plug.

Tighten
Tighten the oil pressure test plug to 11 N·m (97 lb. in).

2. Check the transmission fluid level (fill if necessary). Refer to Transmission Fluid Check .
3. Lower the vehicle.