For 1990-2009 cars

### Removal Procedure

1. Remove transmission control lever assembly. Refer to Transmission Control Replacement.
2. Using a suitable tool release the selector lever knob (1) from the control lever assembly.
3. Remove the selector lever retaining screw (1) and lever backing (3).
4. Remove the selector lever metal retaining clip (1).
5. Remove the selector lever spacer
6. Remove the selector lever by sliding upwards off assembly

### Installation Procedure

1. Install the selector lever (1) by sliding down on the assembly.
2. Install the selector lever spacer (2).
3. Install the selector lever metal retainer clip.
4. Install the selector lever backing (3) and retaining screw (1).
5. Install the selector lever release knob into selector lever.
6. Install the transmission control lever assembly. Refer to Transmission Control Replacement.