For 1990-2009 cars

### Removal Procedure

1. Remove the seat belt buckle. Refer to Seat Belt Buckle Pretensioner Replacement .
2. Remove the front seat inner trim (1) to hinge assembly retaining screw (2).
3. Firmly grasped the top of the front seat inner trim (1) and disengage the retaining clip.
4. Remove the front seat cushion inner trim (1).

### Installation Procedure

1. Install the front seat inner trim (1) to the hinge assembly.
2. Install the front seat inner trim (1) retaining screw (2).
3. Install the seat belt Buckle. Refer to Seat Belt Buckle Pretensioner Replacement .