For 1990-2009 cars

### Removal Procedure

1. Remove the outside rearview mirror. Refer to Power Mirror Replacement.
2. Lower the window to the full down position.

Important: Pull the door outer belt sealing strip (1) to detach the door outer belt sealing strip to door retaining clips (2).

3. Remove the door outer belt sealing strip (1) from the door (3).

### Installation Procedure

Important: Push the door outer belt sealing strip (1) to attach the door outer belt sealing strip to door retaining clips (2).

1. Install the door outer belt sealing strip (1) to the door (3).
2. Install the outside rearview mirror. Refer to Power Mirror Replacement.