For 1990-2009 cars

### Removal Procedure

1. Grasp the front of the console compartment (1) and carefully pull away from the headlining assembly.
2. Slide the console compartment (1) in a forward motion to allow the two locator arms to clear the headlining.
3. Disconnect the console compartment (3) electrical connector (2).
4. Disconnect the bluetooth microphone connection (1).
5. Remove the console compartment (3).

### Installation Procedure

1. Connect the bluetooth microphone connection (1).
2. Connect the console compartment (3) electrical connector (1).
3. Insert the two locating arms into the headlining assembly.
4. Carefully push the console compartment (1) into the headlining assembly.
5. Test console compartment for correct operation.