For 1990-2009 cars

## Transmission Support Replacement Except 5L40 and 6L50

### Removal Procedure

Caution: Refer to Safety Glasses Caution in the Preface section.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the exhaust system. Refer to Exhaust System Replacement.
3. Remove the transmission support to transmission mount retaining nuts.
4. Support the transmission with a suitable supporting stand.
5. Remove the transmission support to lower sub frame rail retaining bolts.
6. Remove the transmission support from the vehicle.

### Installation Procedure

1. Install the transmission support to the vehicle.
2. Install the transmission support to lower sub frame rail retaining bolts.

Notice: Refer to Fastener Notice in the Preface section.

3. Tighten the transmission support to under body retaining bolts.

Tighten
Tighten the bolts to 55 N·m (41 lb ft).

4. Remove the suitable supporting stand from the transmission.
5. Install the transmission support to transmission mount retaining nuts.

Tighten
Tighten the nuts to 25 N·m (18 lb ft).

6. Install the exhaust system. Refer to Exhaust System Replacement.
7. Lower the vehicle.