For 1990-2009 cars

#### Tools Required

• | DT-47721 Shift Shaft Seal Installer

• | J 2619-01 Slide Hammer

• | J 26941 Bushing and Bearing Remover 3 - 4 in

1. Using J 2619-01 and J 26941 , remove the rear output shaft seal (1) from the extension housing.
2. Using J 2619-01 and J 26941 , remove the rear output shaft bearing assembly (1 and 2) from the extension housing.
3. Using tool DT-47721 , remove the shift shaft seal (1) from the extension housing.