For 1990-2009 cars

## Air Inlet Valve Actuator Replacement RHD

### Removal Procedure

1. Remove the I/P lower trim plate assembly. Refer to Instrument Panel Insulator Panel Replacement - Left Side.
2. Remove the I/P compartment assembly. Refer to Instrument Panel Compartment Replacement.
3. Disconnect the recirculation actuator electrical connector (1).
4. Remove the recirculation actuator to HVAC module assembly retaining screws (2).
5. Remove the recirculation actuator (1) from the HVAC module assembly (3).
6. Inspect air intake door shaft end for damage, also check the air intake door for full movement, open/close. If damage is evident, replace the air intake housing. Refer to Air Inlet Assembly Replacement.

### Installation Procedure

1. Align the actuator drive gear (1) with the door shaft spline (2).
2. Install the air intake recirculation actuator (1) to the HVAC module assembly (3).

Notice: Refer to Fastener Notice in the Preface section.

3. Install the recirculation actuator to HVAC module assembly retaining screws (2).

Tighten
Tighten the screws to 1.2 N·m (9 lb ft).

4. Connect the recirculation actuator electrical connector (1).
5. Install the I/P lower trim plate assembly. Refer to Instrument Panel Insulator Panel Replacement - Left Side.
6. Install the I/P compartment assembly. Refer to Instrument Panel Compartment Replacement.
7. Perform HVAC system relearn. Refer to HVAC Control Module Programming and Setup.