For 1990-2009 cars

### Removal Procedure

1. Turn the ignition OFF.
2. Remove the camshaft position (CMP) sensor electrical connector (1) from the CMP sensor (2).
3. Remove the the CMP sensor to engine front cover retaining bolt (1).
4. Remove the CMP sensor from the engine front cover (2).

### Installation Procedure

1. Install the CMP sensor (2) to the engine front cover.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the CMP sensor to engine front cover retaining bolt (1).

Tighten
Tighten the bolt to 10 N·m (89 lb in).

3. Install the CMP sensor electrical connector (1) to the CMP sensor.