For 1990-2009 cars

Notice: Refer to Fastener Notice in the Preface section.

Important: If the pressure test plug (40), O-ring (66), level hole plug (36) and O-ring (37) are not damaged, they should be reused.

1. Inspect the pressure test hole plug (40) and O-ring seal (66) for damage.
2. Install the pressure test plug (40) and O-ring seal (66).

Tighten
Tighten the pressure test plug to 11N·m (8 lb. ft).

3. Inspect the fluid level hole plug (36) and O-ring seal (37) for damage.
4. Install the transmission fluid level hole plug O-ring seal (37) and the transmission fluid level hole plug (36).

Tighten
Tighten the level hole plug to 20N·m (15 lb. ft).