For 1990-2009 cars

1. Install the power steering pump bracket (2).
2. Install the NEW power steering bracket to cylinder head retaining bolts (1).

Tighten
Tighten the bolts to 58 N·m (43 lb ft).

3. Install the power steering fluid reservoir bracket (4).
4. Install the NEW power steering fluid reservoir bracket to engine front cover retaining bolts (3).

Tighten
Tighten the bolts to 9 N·m (80 lb ft).

5. Install the power steering pump (2) to the power steering pump mounting bracket (3).
6. Install the power steering pump to mounting bracket retaining bolts (1).