For 1990-2009 cars

### Removal Procedure

1. Remove the I/P trim panel. Refer to Instrument Panel Trim Panel Replacement.
2. Grasp the lower area of the instrument panel outer cover (1) and carefully pull to disengage the retaining clips (2). The left side is shown, the right side is similar.
3. Remove the instrument panel outer cover (1) rotating upwards to disengage remaining clip (2).

### Installation Procedure

1. Align the instrument panel outer cover (1) to the I/P and correctly locate the upper clips (2).
2. Install the instrument panel outer cover (1) to the I/P by disengaging the retaining clips (2).
3. Install the I/P trim panel. Refer to Instrument Panel Trim Panel Replacement.
4. Ensure all clips are installed correctly.