For 1990-2009 cars

## Clutch Pedal Spongy Low Pedal Effort LHD

#### Clutch Pedal Spongy Low Pedal Effort

Cause | Action
--- | ---
DEFINITION: The clutch pedal may feel spongy, or it requires very little effort to operate. Review Symptoms - Clutch.
Air in the hydraulic system | Bleed the clutch hydraulic system. Refer to Hydraulic Clutch Bleeding.
Master cylinder fluid level low |

1. Inspect for leakage in the clutch master cylinder, hose connections and the clutch actuator.
2. Repair or replace any faulty components.

Incomplete pedal return |

1. Inspect the pedal for full return.
2. Clear any obstacles that may interfere with the pedal operation.

Clutch incorrectly installed | Replace the clutch assembly. Refer to Clutch Assembly Replacement.
Clutch mounting bolts loose or broken |

1. Remove the broken bolts.
2. Replace the broken or loose bolts, and tighten. Refer to Clutch Assembly Replacement.

Clutch pressure plate not adjusted | Adjust the clutch pressure plate. Refer to Clutch Pressure Plate Adjustment.
Release bearing worn or damaged | Replace the release bearing. Refer to Clutch Concentric Actuator Cylinder Replacement.
Contaminated hydraulic fluid |

1. Inspect the clutch hydraulic fluid for contamination of moisture.
2. Inspect the reservoir cap for being faulty if moisture is present.
3. Inspect the clutch hydraulic fluid for dirt or debris.
4. Flush and bleed the clutch hydraulic system if the above conditions are found. Refer to Hydraulic Clutch Bleeding.