For 1990-2009 cars

### Removal Procedure

1. Remove the air cleaner intake duct. Refer to Air Cleaner Inlet Duct Replacement.
2. Release the air cleaner cover retaining clips (1) and remove the air cleaner element from the air filter assembly.

### Installation Procedure

1. Install the air cleaner element (1) to the air cleaner assembly.
2. Install the air cleaner cover retaining clips (1) .
3. Install the air cleaner intake duct. Refer to Air Cleaner Inlet Duct Replacement.