For 1990-2009 cars

#### Tools Required

J 25025-5 Guide Pins

1. Inspect the valve body spacer plate and the solenoid screens (49, 50) for damage or debris.

Replace the solenoid screens (49, 50) if necessary.

2. Install the #1 checkball into the case.
3. Install the J 25025-5 into the case.

Important: M33 models use a bonded spacer plate (48).

4. Place the spacer plate to case gasket (47) (identified by a "C") and the spacer plate to valve body gasket (52) (identified by a "V") on the spacer plate (48). Retain gaskets on the spacer plate with J 36850 or equivalent.
5. Place the spacer and the spacer plate gaskets on the case.
6. Install the spacer plate support plate (53 or 113).
7. Install the spacer plate support retaining bolts (77).

Notice: Refer to Fastener Notice in the Preface section.

8. Install the accumulator retaining bolt (115), model dependent.

Tighten
Tighten the accumulator retaining bolt to 11 N·m (8.11 lb ft).

9. Install the 1-2 accumulator housing assembly (57 or 116).
10. Install the 1-2 accumulator housing retaining bolts (58, 59 or 117, 118).

Tighten
Tighten the retaining bolts 58 and 59 to 11 N·m (8 lb ft).

Tighten
Tighten the retaining bolts 117 and 118 to 8-14 N·m (6-10 lb ft).