For 1990-2009 cars

### Removal Procedure

1. Remove the engine covers. Refer to Engine Cover Replacement.
2. Remove the spark plugs in order to ease crankshaft/engine rotation. Refer to Spark Plug Replacement.
3. Remove the engine front cover. Refer to Engine Front Cover Replacement.
4. Remove the left bank secondary camshaft drive chain tensioner. Refer to Secondary Camshaft Drive Chain Tensioner Removal - Left Side.

### Installation Procedure

1. Install the left bank secondary camshaft drive chain tensioner. Refer to Secondary Camshaft Drive Chain Tensioner Installation - Left Side.
2. Install the spark plugs. Refer to Spark Plug Replacement.
3. Install the engine front cover. Refer to Engine Front Cover Replacement.
4. Install the engine covers. Refer to Engine Cover Replacement.