For 1990-2009 cars

### Removal Procedure

Caution: Refer to Vehicle Lifting Caution in the Preface section.

Caution: Refer to Safety Glasses Caution in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the front wheel. Refer to Tire and Wheel Removal and Installation.
3. Remove the front wheelhouse liner. Refer to Front Wheelhouse Liner Replacement.
4. Remove the side indicator. Refer to Repeater Lamp Replacement.
5. Remove the front fender sound insulator (1) from the vehicle.

### Installation Procedure

1. Install the front fender sound insulator (1) to the vehicle.
2. Install the side indicator. Refer to Repeater Lamp Replacement.
3. Install the front wheelhouse liner. Refer to Front Wheelhouse Liner Replacement.
4. Install the front wheel. Refer to Tire and Wheel Removal and Installation.
5. Lower the vehicle.