For 1990-2009 cars

## Radio Front Speaker Replacement RHD

### Removal Procedure - Tweeter

1. Remove the left instrument panel (I/P) defroster grille. Refer to Defroster Grille Replacement .
2. Remove the tweeter speaker to I/P attaching screw (2).
3. Disconnect the electrical connector (3).

### Installation Procedure - Tweeter

1. Connect the electrical connector (3).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the tweeter speaker to I/P attaching screw (2).

Tighten
Tighten the screw to 2 N·m (18 lb in).

3. Install the left instrument panel defroster grille. Refer to Defroster Grille Replacement .

### Removal Procedure - Center

1. Remove the instrument panel (I/P) defroster grilles. Refer to Defroster Grille Replacement .
2. Remove the upper instrument panel (I/P) center trim. Refer to Instrument Panel Upper Trim Panel Replacement
3. Remove the centre speaker to instrument panel attaching screws (2).
4. Disconnect the electrical connector (3).

### Installation Procedure - Center

1. Connect the electrical connector (3).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the centre speaker to instrument panel attaching screws (2).

Tighten
Tighten the screws to 2 N·m (18 lb in).

3. Install the upper instrument panel (I/P) centre trim. Refer to Instrument Panel Upper Trim Panel Replacement
4. Install the instrument panel defroster grilles. Refer to Defroster Grille Replacement .