For 1990-2009 cars

## Instrument Cluster Trim Panel Replacement SWB

### Removal Procedure

1. Remove the upper instrument cluster trim panel to I/P trim pad retaining screws (1).
2. Remove the lower instrument cluster to I/P pad retaining screws (1), located on either side of the instrument cluster trim panel.
3. Using a suitable tool, carefully remove the top of the trim panel toward the steering wheel.
4. Remove the instrument cluster trim panel.

### Installation Procedure

1. When installing the instrument cluster trim panel, make sure the locating lugs (1) are correctly located.
2. Install the instrument cluster trim panel.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the lower instrument cluster trim panel to I/P pad retaining screws (1).

Tighten
Tighten the screws (1) to 2 N·m (18 lb in).

Notice: Refer to Fastener Notice in the Preface section.

4. Install the upper instrument cluster trim panel to I/P trim pad retaining screws (1).

Tighten
Tighten the screws (1) to 2 N·m (18 lb in).