For 1990-2009 cars

Important:

• | Do not use the crankshaft oil seal again. Install a NEW crankshaft oil seal during assembly.

• | Do not use the front cover-to-engine block gasket again. Install a NEW gasket during assembly.

1. Remove the crankshaft oil seal (140) from the front cover.
2. Clean the cover in solvent. Remove the sealant from the cover oil pan surface. Refer to Replacing Engine Gaskets.

Caution: Refer to Safety Glasses Caution in the Preface section.

3. Dry the cover with compressed air.
4. Inspect the gasket sealing surfaces for above acceptable scratches or gouging.
5. Inspect the threaded bolt holes for damaged threads or debris.
6. Inspect the crankshaft oil seal and camshaft position (CMP) sensor mounting bores for damage.