For 1990-2009 cars

1. Clean the shift shaft and fork assembly parts with a suitable solvent. Air dry all the parts.
2. Inspect the shift forks and the shift links for excessive wear, fractures or distortion.
3. Inspect the shift shaft lever bushings for excessive wear.
4. Inspect the shift fork nylon inserts (1) for wear.
5. Replace parts that are fractured, excessively worn, or distorted.
6. Replace an excessively worn or burred shift shaft.