For 1990-2009 cars

#### Tools Required

• | DT-47722 Shift Rail Bushing Remover and Installer

• | J 2619-01 Slide Hammer

• | J 26941 Bushing and Bearing Remover 3-4 in

### Rear Case Disassemble

1. Remove the oil trough (1) from the rear case.
2. Remove the counter gear roller bearing retainer to rear case retaining bolt (1).
3. Remove the counter gear roller bearing retainer from the rear case.
4. Remove the gasket (3) from the rear case.
5. Using J 26941 and J 2619-01 , remove the counter gear roller bearing (1) from the rear case.
6. Using DT-47722 , remove the shift shaft bearing (1) from the rear case.

### Middle Case Disassemble

Using DT-47722 , remove the shift shaft bearing (1) from the middle case.

### Clutch Housing Disassemble

Using a suitable tool, remove the input shaft seal (1) from the front case (2).