For 1990-2009 cars

## Turn Signal Switch Replacement RHD

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the battery ground cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the upper and lower steering column trim covers. Refer to Steering Column Trim Covers Replacement.
3. Disconnect the turn signal switch (2) electrical connector (1).
4. Press the retaining tabs (1) on the turn signal switch (2) and pull the turn signal switch assembly away from the steering column.

### Installation Procedure

1. Install the new turn signal (2) switch and push the switch into position until the retaining tabs (1) seat with an audible click.
2. Connect the turn signal switch (2) electrical connector (1).
3. Install the upper and lower steering column trim covers. Refer to Steering Column Trim Covers Replacement.
4. Connect the battery ground cable. Refer to Battery Negative Cable Disconnection and Connection.
5. Check all vehicle lights for correct operation.