For 1990-2009 cars

### Removal Procedure

Caution: Refer to Safety Glasses Caution in the Preface section.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.

Important: Nuts with micro-encapsulated thread sealant must be discarded after removal.

2. Remove the stabliser bar insulator bracket to subframe retaining nuts (3) on both sides of the stabiliser bar (4).

Discard the nuts.

3. Remove the stabliser bar insulator bracket (2) from the subframe (1) on both sides of the stabiliser bar.
4. Remove the stabliser bar insulator (2) from both sides of the stabiliser bar (1).
5. Inspect all parts for wear and damage.

### Installation Procedure

1. Install the stabliser bar insulator (2) to both sides of the stabiliser bar (1).
2. Install the stabliser bar insulator bracket (2) to the subframe (1) on both sides of the stabiliser bar.

Notice: Refer to Fastener Notice in the Preface section.

3. Install stabliser bar insulator bracket to subframe retaining nuts (3) on both sides of the stabiliser bar.

Tighten
Tighten the nuts to 22 N·m (16 lb ft).

4. Remove the safety stands.
5. Lower the vehicle to the ground.