For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Bolt M6 x 20 (Quantity: 18)
2 | Fluid Pan Assembly
3 | Fluid Pan Gasket Tip The fluid pan gasket is reusable. Inspect the gasket to determine if it may be reused. If the gasket is stuck to the case or pan, it should be replaced.
4 | Fluid Filter Assembly Notice: Refer to General Repair Instructions in the Preface section.
5 | Fluid Filter Seal Assembly Notice: Refer to General Repair Instructions in the Preface section. Tip Use a screwdriver or snap ring pliers.
6 | Electrical Connector Slide Lock Notice: Refer to General Repair Instructions in the Preface section.
7 | Electrical Connector Passage Sleeve

#### Special Tools

• | DT 47715

• | J 42183