For 1990-2009 cars

## Windshield Wiper Blade Replacement RHD

### Removal Procedure

Important: Ensure that the wiper arms do not interfere with the hood while being moved away from the windshield.

1. Lift the wiper arms (1) away from the windshield to the upright position.

Important: Ensure that the wiper arms remain at rest and Do Not spring back onto the windscreen.

2. Press the wiper arm blade side clip (2) in and unclip the wiper arm (1) blade.
3. Remove the wiper arm blade from the wiper arm (1).

### Installation Procedure

1. Clip the wiper arm blade connector onto the wiper arm. Listen for an audible click to confirm fitting.
2. Move the wiper arm back to the parked position.
3. Test the windshield wipers and washers for correct operation.