For 1990-2009 cars

Note: Review the system operation in order to familiarize yourself with the system functions. Refer to Object Detection Description and Operation.

### Visual/Physical Inspection

• | Inspect for aftermarket devices which could affect the operation of the system. Refer to Checking Aftermarket Accessories

• | Inspect the easily accessible or visible system components for obvious damage or conditions which could cause the symptom.

• | Make sure the rear object alarm sensors located on the vehicles rear bumper are clear. Remove any snow, mud, or ice that is blocking the sensors.

• | If the vehicle is fitted with a trailer hitch, enter the customisation menu in the infotainment unit and select Tow Bar Att . Select Yes if a tow ball tongue/neck is attached or No if a tow ball tongue/neck is removed.

• | Drive the vehicle for longer than 20 seconds and at a speed greater than 17km/h.

### Intermittent

Faulty electrical connections or wiring may be the cause of intermittent conditions. Refer to Testing for Intermittent Conditions and Poor Connections.

### Symptom List

Rear Parking Assist Malfunction