For 1990-2009 cars

### Removal Procedure

Important: Protect the paint and body work with tape or a clean cloth. Failure to do so may result in damage to the paint work.

Important: Using a suitable tool pry the roof weld joint reveal moulding (1) from the roof weld joint (3) starting at the front of the vehicle at points close to the roof weld joint reveal moulding retaining clips (2).

1. Remove the roof weld joint reveal moulding (1) from the roof weld joint (3) by lifting the front edge of the roof weld joint reveal moulding upwards and slide from underneath the rear header trim.

Important: Clean the surface with a suitable cleaning solution and a lint free cloth to remove any dirt or debris from the roof weld joint (3).

2. Remove any dirt or debris from the roof weld joint (3).

### Installation Procedure

Important: If the roof weld joint reveal moulding or roof weld joint reveal moulding retaining clips are cracked, broken or are damaged in anyway, replace the damaged component.

Important: Position the roof weld joint reveal moulding under the rear header trim prior to installation.

1. Make sure the front edge of the roof weld joint reveal moulding (1) is located correctly under the top edge of the front windshield seal (2).
2. Align the roof weld joint reveal moulding retaining clips (2) in the correct position and push firmly into place engaging the roof weld joint reveal moulding retaining clips into the body.