For 1990-2009 cars

The purpose of the brake warning system is to warn the driver of a electronic brake deferential (EBD) failure and/or a low brake fluid condition. It also alerts the driver that the park brake is applied whilst the vehicle is being driven.

• | A brake EBD fail warning is active when the brake fail signal is active.

| A red telltale illuminates whilst the brake fail signal is active.

| A brake EBD Fail Warning is displayed both as an animation on the multi function display (MFD) and as a telltale. The general warning chime sounds when the animated warning activates. The chime will not repeat whilst the warning remains active.

| The brake EBD fail warning remains on the MFD until:

- | The ENTER switch is pressed.

- | The TRIP button is pressed.

- | The condition is rectified.

• | A brake fluid level warning is active when the instrument panel cluster (IPC) detects an increase in resistance in the brake fluid level switch circuit.

| A red telltale illuminates continuously with the ignition ON and when the resistance of the brake fluid level switch circuit is above a predetermined value.

| The brake fluid level warning is displayed both as an animation on the MFD and as a telltale. The general warning chime sounds when the animated warning activates. The chime will not repeat whilst the warning remains active.

| The brake fluid level warning remains on the MFD until:

- | The ENTER switch is pressed.

- | The TRIP button is pressed.

- | The condition is rectified.

• | The park brake warning is active when the park brake signal is active and the vehicle speed is greater than 10 km/h (6 mph).

| A red telltale illuminates whilst the park brake signal is active, regardless of the vehicle speed.

| The Park Brake Warning is displayed both as an animation on the MFD and as a telltale. The general warning chime sounds when the animated warning activates. The chime will not repeat whilst the warning remains active.

| The park brake warning remains on the MFD until:

- | The ENTER switch is pressed.

- | The TRIP button is pressed.

- | The condition is rectified.

- | The speed is reduced to less than 10 km/h (6 mph).