For 1990-2009 cars

The mechanical components of the 6-Speed RWD are as follows:

• | A torque converter with an electronically controlled capacity clutch (ECCC)

• | Vane-type fluid pump assembly

• | 1-2-3-4 and 3-5 Reverse clutch assembly

• | Input sun gear and carrier assembly

• | 4-5-6 clutch assembly with turbine shaft

• | 4-5-6 clutch hub assembly

• | 1-2-3-4 clutch hub assembly

• | 2-6 and 3-5 reverse clutch hub assembly

• | Centre support assembly, with 2-6 clutch assembly, and low and Reverse clutch assembly

• | Low clutch sprag assembly

• | A double planetary output carrier assembly

• | Output shaft assembly

• | Control valve body assembly

The electrical components of the 6-Speed RWD are as follows:

• | Input and output speed sensor assembly

• | Manual shift shaft position switch

• | Control solenoid valve assembly, which contains the following components:

- | Transmission control module (TCM)

- | 5 variable bleed line pressure control (PC) solenoids

- | Transmission fluid pressure (TFP) switch assembly

- | Torque converter clutch (TCC) pressure control solenoid

- | 2 shift solenoids

For more information, refer to Electronic Component Description .