For 1990-2009 cars

### Removal Procedure

Caution: Refer to Safety Glasses Caution in the Preface section.

1. Turn the ignition OFF.
2. Disconnect the purge line (1) from the purge valve solenoid.
3. Disconnect the purge valve solenoid electrical connector (1).
4. Disconnect the purge line (1) from the manifold side of the purge valve solenoid.
5. Remove the purge valve solenoid.

### Installation Procedure

1. Install the purge valve solenoid.
2. Connect the purge line (1) from the manifold side of the purge valve solenoid.
3. Connect the purge valve solenoid electrical connector.
4. Connect the purge line (1) to the purge valve solenoid.