For 1990-2009 cars

### Removal Procedure

Caution: Refer to Exhaust Service Caution in the Preface section.

1. Remove the rear Insulator hanger to body retaining bolts (1).
2. Remove the rear insulator hanger (1) from the rear muffler (2).

### Installation Procedure

1. Install the rear insulator hanger (1) to the rear muffler (2).
2. Install the rear insulator hanger to body retaining bolts (1).

Tighten
Tighten the bolts to 26 N·m (19 lb ft).