For 1990-2009 cars

#### Tools Required

• | J 8092 Drive Handle

• | J 44765 Seal Installer

• | J 39546 Bearing Race Installer

• | J 39437 Bushing Installer

1. Install the mainshaft bearing race (1), using the J 39546 (2) and the J 8092 (3).
2. Install the mainshaft bearing race to extension housing retainer ring (1).
3. Install a NEW output shaft seal to the extension housing using the J 44765 .
4. Apply an approved sealant to the transmission case drain plug.

Notice: Refer to Fastener Notice in the Preface section.

5. Install the transmission case drain plug (1) to the extension housing.

Tighten
Tighten the plug to 18 N·m (13 Ib ft).