For 1990-2009 cars

### Removal Procedure

1. Remove the door upper auxiliary weatherstrip. Refer to Front Side Door Upper Auxiliary Weatherstrip Replacement .
2. Detach the door frame garnish molding locking tab (1) from the door frame (2) using a suitable flat bladed tool.
3. Remove the door frame garnish molding (1) from the door (2).

### Installation Procedure

1. Position the door frame garnish molding (1) to the door (2).

Important: Push the door frame garnish molding until the locking tab (1) locates in the door frame (2).

2. Attach the door frame garnish molding locking tab (1) to the door frame (2).
3. Install the door upper auxiliary weatherstrip. Refer to Front Side Door Upper Auxiliary Weatherstrip Replacement .