For 1990-2009 cars

#### Transmission Overheats

Checks | Causes
--- | ---
TCC Circuit | Blockage during apply or release
Pump Cover (215) | Cross channel leakage
Pressure Regulator Valve (216) | The valve is stuck in a high demand position
Oil Cooler | The cooler or the cooler lines are blocked
Oil Pan Gasket (73) | The gasket is damaged
Turbine Shaft O-ring (618) | The O-ring is damaged
Turbine Shaft Seals (619) | The seals are damaged
Stator Shaft Bushings (234/241) | The bushing is worn or damaged
Fluid | The fluid level is low
Radiator | Air flow is restricted or internal blockage