For 1990-2009 cars

### Removal Procedure

1. Remove the cargo liner. Refer to Cargo Box Liner Replacement .
2. Remove the rear body rail end cover. Refer to Pickup Box Cover Side Rail End Cover Replacement .
3. Remove the cargo tie down plates. Refer to Cargo Tie Down Loop Bracket Replacement .
4. Remove the rear body rail cover to body retaining bolts (1).
5. Remove the rear body rail cover (2) from the vehicle (3).

### Installation Procedure

1. Install the rear body rail cover (2) to the vehicle (3).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the rear body rail cover to body retaining bolts (1).

Tighten
Tighten the bolts to 6 N·m (53 lb in).

3. Install the rear body rail end cover. Refer to Pickup Box Cover Side Rail End Cover Replacement .
4. Install the cargo tie down plates. Refer to Cargo Tie Down Loop Bracket Replacement .
5. Install the cargo liner. Refer to Cargo Box Liner Replacement .