For 1990-2009 cars

This master DTC list includes all applicable DTCs in alphanumeric order with descriptors.

DTC | DTC Descriptor | Module That Sets the DTC | Diagnostic Procedure
--- | --- | --- | ---
B0012 | Driver Frontal Deployment Loop Stage 1 | SDM | DTC B0012 or B0013
B0013 | Driver Frontal Deployment Loop Stage 2 | SDM | DTC B0012 or B0013
B0015 | Driver Pretensioner Deployment Stage 1 Loop | SDM | DTC B0015
B0019 | Passenger Frontal Deployment Loop Stage 1 | SDM | DTC B0019 or B0020
B0020 | Passenger Frontal Deployment Loop Stage 2 | SDM | DTC B0019 or B0020
B0022 | Passenger Pretensioner Deployment Stage 1 Loop | SDM | DTC B0022
B0052 | Deployment Commanded | SDM | DTC B0052 or B0053
B0053 | Deployment Commanded with Loop DTCs Present | SDM | DTC B0052 or B0053
B0072 | Driver Seat Belt Sensor Circuit | SDM | DTC B0072
B0079 | Driver Seat Position Sensor Circuit | SDM | DTC B0079
B0083 | Front End Sensor 1 | SDM | DTC B0083 or B0084
B0084 | Front End Sensor 2 | SDM | DTC B0083 or B0084
B013B | Coil Compressor Stroke Control Circuit | HVAC | DTC B013B
B0158 | Outside Air Temperature Sensor Circuit | HVAC | DTC B0158 or B0168
B0168 | Passenger Compartment Temperature Sensor Circuit | HVAC | DTC B0158 or B0168
B0183 | Left Solar Load Sensor 1 Circuit | HVAC | DTC B0183 or B0188
B0188 | Right Solar Load Sensor 2 Circuit | HVAC | DTC B0183 or B0188
B0193 | Blower Motor Feedback Circuit | HVAC | DTC B0193
B0198 | Blower Motor Feedback Circuit | HVAC | DTC B0198 2
B0228 | Air Intake Flow Actuator Fault (LHD) or Recirculation Door Motor Circuit (RHD) | HVAC | DTC B0228, B0238, B0253, B0408, B0418, B0428, or B3531
B0238 | Demist Actuator Fault (LHD) or Defogger Door Motor Circuit (RHD) | HVAC | DTC B0228, B0238, B0253, B0408, B0418, B0428, or B3531
B0253 | Face/Floor Actuator Fault (LHD) or Vent/Floor Door Motor Circuit (RHD) | HVAC | DTC B0228, B0238, B0253, B0408, B0418, B0428, or B3531
B0283 | Electric Rear Defrost Circuit | HVAC | DTC B0283
B0408 | Drivers Side Air Mix Actuator (LHD) or Drivers Air Mix Door Motor Circuit (RHD) | HVAC | DTC B0228, B0238, B0253, B0408, B0418, B0428, or B3531
B0418 | Passenger Side Air Mix Actuator (LHD) or Passengers Air Mix Door Motor Circuit (RHD) | HVAC | DTC B0228, B0238, B0253, B0408, B0418, B0428, or B3531
B0428 | Rear Air Mix Door Motor Circuit | HVAC | DTC B0228, B0238, B0253, B0408, B0418, B0428, or B3531
B0958 | Park Assist Sensor Rear Left Outer Circuit | UPA | DTC B0958, B0959, B0960, or B0961
B0959 | Park Assist Sensor Rear Left Middle Circuit | UPA | DTC B0958, B0959, B0960, or B0961
B0960 | Park Assist Sensor Rear Right Middle Circuit | UPA | DTC B0958, B0959, B0960, or B0961
B0961 | Park Assist Sensor Rear Right Outer Circuit | UPA | DTC B0958, B0959, B0960, or B0961
B0970 | Hazard Warning Switch Stuck | BCM | DTC B0970
B0983 | Security System Indicator 2 Circuit | BCM | DTC B0983
B0996 | Vehicle Identification Number Mismatch | Radio, RSE | DTC B0996, 1016, or B1271
B0997 | Auxiliary Electronic Control Unit (ECU) 2 Performance | Radio | DTC B0997
B1000 | Electronic Control Unit (ECU) Performance | BCM, IPC, MSM, RFA, SDM, TDM, Telematics, UPA | DTC B1000
B1001 | Option Configuration Error | BCM, IPC | DTC B1001
SDM | DTC B1001
B1008 | Calibration Data Not Programmed | BCM | DTC B1008
B1010 | System Sensor Data Mismatch Invalid Odometer Signal | NIM | DTC B1010
B1011 | System Disabled Over Temperature | NIM | DTC B1011
B1016 | Vehicle Identification Number (VIN) Not Programmed | BCM | DTC B1016
Radio | DTC B0996, 1016, or B1271
SDM | DTC B1016
B1019 | System Configuration Error | Radio | DTC B1019
B101D | ECU Hardware Performance | BCM, NIM, Radio, RSE, | DTC B101D
B101E | ECU Software Performance | Radio | DTC B101E
B1020 | Auxiliary Electronic Unit (ECU) Performance | NIM | DTC B1020
B1023 | Integral Switch Performance | Radio | DTC B1023
B1024 | Printed Circuit Board (PCB) Temperature Sensor Fault | IPC | DTC B1024
B1025 | Audio Output 1 Left Front Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1035 | Audio Output 2 Right Front Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1045 | Audio Output 3 Left Rear Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1055 | Audio Output 4 Right Rear Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1240 | CD-Player Malfunction | Radio | DTC B1240 or B1245
B1243 | CD-Player Load or Eject Malfunction | Radio | DTC B1243 or B1248
B1244 | CD-Player, Disc Upside Down | Radio | DTC B1244 or B1249
B1245 | CD-Changer Malfunction | Radio | DTC B1240 or B1245
B1248 | CD Changer Load/Unload Performance | Radio | DTC B1243 or B1248
B1249 | CD-Changer, Disc Upside Down | Radio | DTC B1244 or B1249
B1271 | Theft Locked | Radio | DTC B0996, 1016, or B1271
B1325 | Device Power Circuit | HVAC | DTC B1325
B1370 | Device Ignition 1 Circuit | BCM, MSM | DTC B1370-B1379, B1380-B1389, or B1440-B1443
SDM | DTC B1370
B1380 | Device Ignition ACCESSORY Circuit | BCM | DTC B1370-B1379, B1380-B1389, or B1440-B1443
B138A | Device Voltage Reference Group 1 Outputs | UPA | DTC B138A
B1428 | Ignition Switched Power Relay 1 Circuit | BCM | DTC B1428
B1433 | Ignition Switched Power Relay 2 Circuit | BCM | DTC B1433
B1440 | Power Mode Master Input Circuit Malfunction | BCM | DTC B1370-B1379, B1380-B1389, or B1440-B1443
B1441 | Device Ignition OFF, RUN, and CRANK Circuit | BCM | DTC B1370-B1379, B1380-B1389, or B1440-B1443
B1475 | Retained Accessory Power Circuit | BCM | DTC B1475
B1516 | Battery Current Sensor Performance | BCM | DTC B1516
B1517 | Battery Voltage | BCM | DTC B1517
B1527 | High Parasitic Load Detected | BCM | DTC B1527
B2461 | Navigation Electronic Control Unit (ECU) Synchronous Signal Error | NIM | DTC B2461
B2462 | Global Positioning System (GPS) Antenna Circuit | NIM, Telematics | DTC B2462
B2464 | Navigation Player Decoding Error | Radio | DTC B2464
B2484 | Global Positioning System Sensor Open Circuit | NIM | DTC B2484
B2530 | Front Foglamps Control Circuit | BCM | DTC B2530
B2545 | Backup Lamps Circuit | BCM | DTC B2545
B2555 | Passenger Compartment Lamp Control Circuit | BCM | DTC B2555
B2575 | Headlamp Low Beam Control Circuit | BCM | DTC B2575
B257A | Headlamp Switch Input Signals Mismatch | BCM | DTC B257A
B2580 | Headlamp High Beam Control Circuit | BCM | DTC B2580
B2585 | Parklamp Control Circuit | BCM | DTC B2585
B2610 | Passenger Compartment Dimming 1 Circuit | BCM | DTC B2610
B2615 | Passenger Compartment Dimming 2 Circuit | BCM | DTC B2615
B2625 | Display Dimming Pulse Width Modulation (PWM) Output Circuit | BCM | DTC B2625
B2645 | Ambient Light Sensor Circuit | BCM | DTC B2645
B2652 | Passenger Compartment Dimming 3 Circuit | BCM | DTC B2652
B2705 | Gearshift Unlock Circuit | BCM | DTC B2705
B2730 | Interior Trunk/Liftglass/Hatch Release Switch Circuit | BCM | DTC B2730
B2745 | Traction Control Switch Circuit | BCM | DTC B2745
B2750 | Horn Relay Coil Circuit | BCM | DTC B2750
B2815 | Steering Wheel Switch Circuit | IPC | DTC B2815
B2976 | Driver Door Ajar Circuit | BCM | DTC B2976
B2991 | Passenger Door Ajar Circuit | BCM | DTC B2991
B3006 | Hood Ajar Circuit Plausability Failure | BCM | DTC B3006
B3055 | No Transponder Modulation or No Transponder | TDM | DTC B3055
B3060 | Unprogrammed Transponder Key Identification Code Received | TDM | DTC B3060
B3105 | Keyless Entry System Key Not Programmed | RFA | DTC B3105
B3109 | Keyless Entry Transmitter 1 Battery Low Voltage | RFA | DTC B3109
B3110 | Keyless Entry Transmitter 2 Battery Low Voltage | RFA | DTC B3110
B3111 | Keyless Entry Transmitter 3 Battery Low Voltage | RFA | DTC B3111
B3112 | Keyless Entry Transmitter 4 Battery Low Voltage | RFA | DTC B3112
B3125 | Left Front/Driver Door Only Unlock Circuit | BCM | DTC B3125, B3130, or B3135
B3130 | All Door Unlock Circuit | BCM | DTC B3125, B3130, or B3135
B3135 | All Door Lock Circuit | BCM | DTC B3125, B3130, or B3135
B3140 | Driver Unlock Switch Circuit | BCM | DTC B3140 or B3150
B3150 | Driver Lock Switch Circuit | BCM | DTC B3140 or B3150
B3265 | Trunk/Hatch/Liftglass Release Output Circuit | BCM | DTC B3265
B3445 | Stop Lamp Circuit | BCM | DTC B3445
B3531 | Rear Air Mode Door Motor Circuit | HVAC | DTC B0228, B0238, B0253, B0408, B0418, B0428, or B3531
B3715 | Front Wiper Relay Drive Circuit | BCM | DTC B3715
B3794 | Cruise Control Function Request Circuit | BCM | DTC B3794
B3873 | Front Washer Relay Circuit | BCM | DTC B3873
B3875 | Wiper High Speed Relay Circuit | BCM | DTC B3875
B3933 | Evaporator Temperature Sensor Circuit | HVAC | DTC B3933
B3935 | Transponder Key Identification Error | TDM | DTC B3935
B3976 | Unconfigured Transponder Key | TDM | DTC B3976
C0035 | Front Left Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0040 | Front Right Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0045 | Rear Left Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0050 | Rear Right Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0060 | Left Front Outlet Valve Malfunction | EBCM | DTC C0060-C0095, C0100, C0105, C0121, C0141, C0146, C0151, or C0156
C0065 | Left Front Inlet Valve Malfunction | EBCM | DTC C0060-C0095, C0100, C0105, C0121, C0141, C0146, C0151, or C0156
C0070 | Right Front Outlet Valve Malfunction | EBCM | DTC C0060-C0095, C0100, C0105, C0121, C0141, C0146, C0151, or C0156
C0075 | Right Front Inlet Valve Malfunction | EBCM | DTC C0060-C0095, C0100, C0105, C0121, C0141, C0146, C0151, or C0156
C0080 | Left Rear Outlet Valve Malfunction | EBCM | DTC C0060-C0095, C0100, C0105, C0121, C0141, C0146, C0151, or C0156
C0085 | Left Rear Inlet Valve Malfunction | EBCM | DTC C0060-C0095, C0100, C0105, C0121, C0141, C0146, C0151, or C0156
C0090 | Right Rear Outlet Valve Malfunction | EBCM | DTC C0060-C0095, C0100, C0105, C0121, C0141, C0146, C0151, or C0156
C0095 | Right Rear Inlet Valve Malfunction | EBCM | DTC C0060-C0095, C0100, C0105, C0121, C0141, C0146, C0151, or C0156
C0100 | AR Outlet Valve Malfunction | EBCM | DTC C0060-C0095, C0100, C0105, C0121, C0141, C0146, C0151, or C0156
C0105 | AR Inlet Valve Malfunction | EBCM | DTC C0060-C0095, C0100, C0105, C0121, C0141, C0146, C0151, or C0156
C0110 | Return Pump Circuit Malfunction | EBCM | DTC C0110
C0121 | Valve Relay Circuit Malfunction | EBCM | DTC C0060-C0095, C0100, C0105, C0121, C0141, C0146, C0151, or C0156
C0126 | Low Brake Fluid Indicated | EBCM | DTC C0126
C0131 | Antilock Brake System Pressure Circuit | EBCM | DTC C0131
C0141 | Front Left/Front Right TC/ESP Priming Valve Circuit Malfunction | EBCM | DTC C0060-C0095, C0100, C0105, C0121, C0141, C0146, C0151, or C0156
C0146 | Front Left/Front Right TC/ESP Switch Over Valve Circuit Malfunction | EBCM | DTC C0060-C0095, C0100, C0105, C0121, C0141, C0146, C0151, or C0156
C0151 | Rear Left/Rear Right TC/ESP Priming Valve Circuit Malfunction | EBCM | DTC C0060-C0095, C0100, C0105, C0121, C0141, C0146, C0151, or C0156
C0156 | Rear Left/Rear Right TC/ESP Switch Over Valve Circuit Malfunction | EBCM | DTC C0060-C0095, C0100, C0105, C0121, C0141, C0146, C0151, or C0156
C0161 | Brake Switch Circuit | EBCM | DTC C0161
C0186 | Lateral Accelerometer | ABS | DTC C0186 or C0196
C0196 | Yaw Rate Circuit | ABS | DTC C0186 or C0196
C0245 | Wheel Speed Sensor Frequency | EBCM | DTC C0245
C0252 | Implausible Control | EBCM | DTC C0252
C0277 | Brake Pedal Position Sensor Circuit | BCM | DTC C0277 or C0890
C0297 | Brake Applied Output Circuit | BCM | DTC C0297
C0460 | Steering Angle Sensor Circuit | EBCM | DTC C0460
C0561 | CAN-Bus Invalid Data | EBCM | DTC C0561
C0565 | Vehicle Identification Number (VIN) Not Programmed/Mismatch | EBCM | DTC C0565
C0569 | System Configuration Error | EBCM | DTC C0569
C0890 | Device Voltage Reference Output 3 Circuit | BCM | DTC C0277 or C0890
C1209 | Left Rear Wheel Speed Sensor Circuit High | EBCM, ECM | DTC C1209, C1223, C1227, or C1234
C1210 | Right Rear Wheel Speed Sensor Circuit High | EBCM, ECM | DTC C1210, C1224, C1228, or C1235
C1223 | Left Rear Wheel Speed Sensor Circuit | EBCM, ECM | DTC C1209, C1223, C1227, or C1234
C1224 | Right Rear Wheel Speed Sensor Circuit | EBCM, ECM | DTC C1210, C1224, C1228, or C1235
C1227 | Left Rear Wheel Speed Sensor Circuit Range/Performance | EBCM, ECM | DTC C1209, C1223, C1227, or C1234
C1228 | Right Rear Wheel Speed Sensor Circuit Range/Performance | EBCM, ECM | DTC C1210, C1224, C1228, or C1235
C1234 | Left Rear Wheel Speed Sensor Circuit Low | EBCM, ECM | DTC C1209, C1223, C1227, or C1234
C1235 | Right Rear Wheel Speed Sensor Circuit Low | EBCM, ECM | DTC C1210, C1224, C1228, or C1235
P0008 | Engine Position System Performance Bank 1 | ECM | DTC P0008 or P0009
P0009 | Engine Position System Performance Bank 2 | ECM | DTC P0008 or P0009
P0010 | Intake Camshaft Position Control Solenoid Circuit Malfunction Bank 1 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P0011 | Intake Camshaft Position Range/Performance Bank 1 | ECM | DTC P0011, P0014, P0021, or P0024
P0013 | Exhaust Camshaft Position Control Solenoid Circuit Malfunction Bank 1 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P0014 | Exhaust Camshaft Position Range/Performance Bank 1 | ECM | DTC P0011, P0014, P0021, or P0024
P0016 | Crankshaft/Intake Camshaft Position not Plausible Bank 1 | ECM | DTC P0016, P0017, P0018, or P0019 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Crankshaft Position (CKP) Camshaft Position (CMP) Correlation | DTC P0016 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0017 | Crankshaft/Exhaust Camshaft Position not Plausible Bank 1 | ECM | DTC P0016, P0017, P0018, or P0019
P0018 | Crankshaft/Intake Camshaft Position not Plausible Bank 2 | ECM | DTC P0016, P0017, P0018, or P0019
P0019 | Crankshaft/Exhaust Camshaft Position not Plausible Bank 2 | ECM | DTC P0016, P0017, P0018, or P0019
P0020 | Intake Camshaft Position Control Solenoid Circuit Malfunction Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P0021 | Intake Camshaft Position Range/Performance Bank 2 | ECM | DTC P0011, P0014, P0021, or P0024
P0023 | Exhaust Camshaft Position Control Solenoid Circuit Malfunction Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P0024 | Exhaust Camshaft Position Range/Performance Bank 2 | ECM | DTC P0011, P0014, P0021, or P0024
P0030 | O2 Sensor Heater Circuit Malfunction Bank 1 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
HO2S Heater Control Circuit Bank 1 Sensor 1 | DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine or DTC P0030, P0036, P0050, or P0056 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0031 | O2 Sensor Heater Circuit Low Voltage Bank 1 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0032 | O2 Sensor Heater Circuit High Voltage Bank 1 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0036 | O2 Sensor Heater Circuit Malfunction Bank 1 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
HO2S Heater Control Circuit Bank 2 | DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine or DTC P0030, P0036, P0050, or P0056 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0037 | O2 Sensor Heater Circuit Low Voltage Bank 1 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0038 | O2 Sensor Heater Circuit High Voltage Bank 1 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0040 | O2 Sensor Signals not Plausible Bank 1 Sensor 1 & Bank 2 Sensor 1 | ECM | DTC P0040 or P0041
P0041 | O2 Sensor Signals not Plausible Bank 1 Sensor 2 & Bank 2 Sensor 2 | ECM | DTC P0040 or P0041
P0050 | O2 Sensor Heater Circuit Malfunction Bank 2 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
HO2S Heater Control Bank 2 Sensor 1 | DTC P0050, P0056, P0059, P0060, P0155, or P0161 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine or DTC P0030, P0036, P0050, or P0056 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0051 | O2 Sensor Heater Circuit Low Voltage Bank 2 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0052 | O2 Sensor Heater Circuit High Voltage Bank 2 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0053 | O2 Sensor Heater Resistance Range/Performance Bank 1 Sensor 1 | ECM | DTC P0053 or P0059 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
HO2S Heater Resistance Circuit Bank 1 Sensor 1 | DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine or DTC P0053, P0054, P0059, or P0060 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0054 | HO2S Heater Resistance Circuit Bank 1 Sensor 2 | ECM | DTC P0030, P0036, P0053, P0054, P0135, or P0141
P0056 | O2 Sensor Heater Circuit Malfunction Bank 2 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
HO2S Heater Control Bank 2 Sensor 2 | DTC P0050, P0056, P0059, P0060, P0155, or P0161 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine or DTC P0030, P0036, P0050, or P0056 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0057 | O2 Sensor Heater Circuit Low Voltage Bank 2 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0058 | O2 Sensor Heater Circuit High Voltage Bank 2 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0059 | O2 Sensor Heater Resistance Range/Performance Bank 2 Sensor 1 | ECM | DTC P0053 or P0059 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
HO2S Heater Resistance Bank 2 Sensor 1 | DTC P0050, P0056, P0059, P0060, P0155, or P0161 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine or DTC P0053, P0054, P0059, or P0060 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0060 | HO2S Heater Resistance Bank 2 Sensor 2 | ECM | DTC P0050, P0056, P0059, P0060, P0155, or P0161 or DTC P0053, P0054, P0059, or P0060 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0068 | Throttle Body Airflow Performance | ECM | DTC P0068 or P0121 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0100 | Mass Air Flow Sensor Circuit Malfunction | ECM | DTC P0100, P0102, or P0103
P0101 | Mass Air Flow Sensor Circuit Range/Performance | ECM | DTC P0101 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Mass Air Flow (MAF) Sensor Performance | ECM | DTC P0101 or P1101 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0102 | Mass Air Flow Sensor Voltage Low | ECM | DTC P0100, P0102, or P0103 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Mass Air Flow (MAF) Sensor Circuit Low Frequency | ECM | DTC P0102 or P0103 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0103 | Mass Air Flow Sensor Voltage High | ECM | DTC P0100, P0102, or P0103 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Mass Air Flow (MAF) Sensor Circuit High Frequency | ECM | DTC P0102 or P0103 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0106 | Manifold Absolute Pressure (MAP) Sensor Performance | ECM | DTC P0106
P0107 | Manifold Absolute Pressure (MAP) Sensor Circuit Low Voltage | ECM | DTC P0107 or P0108
P0108 | Manifold Absolute Pressure (MAP) Sensor Circuit High Voltage | ECM | DTC P0107 or P0108
P0111 | Intake Air Temperature Sensor Circuit Range/Performance | ECM | DTC P0111-P0113
P0112 | Intake Air Temperature Sensor Circuit Low Voltage | ECM | DTC P0111-P0113 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
DTC P0112 or P0113 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0113 | Intake Air Temperature Sensor Circuit High Voltage | ECM | DTC P0111-P0113 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
DTC P0112 or P0113 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0115 | Engine Coolant Temperature (ECT) Sensor Circuit | TCM | DTC P0115, P0120, P0826, P2544, or P2637
P0116 | Engine Coolant Temperature (ECT) Sensor Performance | ECM | DTC P0116 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0116 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0117 | Engine Coolant Temperature (ECT) Sensor Circuit Low Voltage | ECM | DTC P0117 or P0118 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0117 or P0118 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0118 | Engine Coolant Temperature (ECT) Sensor Circuit High Voltage | ECM | DTC P0117 or P0118 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0117 or P0118 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0119 | Engine Coolant Temperature Sensor Circuit Intermittent | ECM | DTC P0119
P0120 | Throttle Position Sensor 1 Circuit | ECM | DTC P0120, P0122, P0123, P0220, P0222, P0223, or P2135 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
Throttle Position (TP) Sensor Circuit | TCM | DTC P0115, P0120, P0826, P2544, or P2637
P0121 | Throttle Position Sensor 1 Circuit Range/Performance | ECM | DTC P0121, P0122, P0123, P0221, P0222, or P0223 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Throttle Position (TP) Sensor 1 Performance | ECM | DTC P0068 or P0121 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0122 | Throttle Position Sensor 1 Circuit Low Voltage | ECM | DTC P0121, P0122, P0123, P0221, P0222, or P0223 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0120, P0122, P0123, P0220, P0222, P0223, or P2135 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0123 | Throttle Position Sensor 1 Circuit High Voltage | ECM | DTC P0121, P0122, P0123, P0221, P0222, or P0223 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0120, P0122, P0123, P0220, P0222, P0223, or P2135 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0125 | Engine Coolant Temperature (ECT) Insufficient for Closed Loop | ECM | DTC P0125
P0128 | Engine Coolant Temperature Below Thermostat Regulating Temperature | ECM | DTC P0128 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0128 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0130 | O2 Sensor Circuit Malfunction Bank 1 Sensor 1 | ECM | DTC P0130 or P0150
P0131 | O2 Sensor Circuit Low Voltage Bank 1 Sensor 1 | ECM | DTC P0131 or P0151 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0131, P0132, P0137, or P0138 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0132 | O2 Sensor Circuit High Voltage Bank 1 Sensor 1 | ECM | DTC P0132 or P0152 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0131, P0132, P0137, or P0138 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0133 | O2 Sensor Circuit Slow Response Bank 1 Sensor 1 | ECM | DTC P0133 or P0153 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0133, P0134, P0140, P1133, P2270, or P2271 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0134 | O2S Circuit Insufficient Activity Bank 1 Sensor 1 | ECM | DTC P0134 or P0154 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0133, P0134, P0140, P1133, P2270, or P2271 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0135 | O2 Sensor Heater Circuit Range/Performance Bank 1 Sensor 1 | ECM | DTC P0135, P0141, P0155, or P0161 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0137 | O2 Sensor Circuit Low Voltage Bank 1 Sensor 2 | ECM | DTC P0137, P0138, P0140, P0157, P0158, or P0160 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0131, P0132, P0137, or P0138 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0138 | O2 Sensor Circuit High Voltage Bank 1 Sensor 2 | ECM | DTC P0137, P0138, P0140, P0157, P0158, or P0160 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0131, P0132, P0137, or P0138 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P013A | HO2S Slow Response Rich to Lean Bank 1 Sensor 2 | ECM | DTC P013A, P013C, P013E, or P014A
P013C | HO2S Slow Response Rich to Lean Bank 2 Sensor 2 | ECM | DTC P013A, P013C, P013E, or P014A
P013E | HO2S Delayed Response Rich to Lean Bank 1 Sensor 2 | ECM | DTC P013A, P013C, P013E, or P014A
P0140 | O2 Sensor Circuit No Activity Detected Bank 1 Sensor 2 | ECM | DTC P0137, P0138, P0140, P0157, P0158, or P0160 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
HO2S Circuit Insufficient Activity Bank 1 Sensor 2 | ECM | DTC P0133, P0134, P0140, P1133, P2270, or P2271 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0141 | O2 Sensor Heater Circuit Range/Performance Bank 1 Sensor 2 | ECM | DTC P0135, P0141, P0155, or P0161 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
HO2S Heater Performance Bank 1 Sensor 2 | ECM | DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P014A | HO2S Delayed Response Rich to Lean Bank 2 Sensor 2 | ECM | DTC P013A, P013C, P013E, or P014A
P0150 | O2 Sensor Circuit Malfunction Bank 2 Sensor 1 | ECM | DTC P0130 or P0150
P0151 | O2 Sensor Circuit Low Voltage Bank 2 Sensor 1 | ECM | DTC P0131 or P0151 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
HO2S Circuit Low Voltage Bank 2 Sensor 1 | DTC P0151, P0152, P0157, or P0158 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0152 | O2 Sensor Circuit High Voltage Bank 2 Sensor 1 | ECM | DTC P0132 or P0152 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
HO2S Circuit High Voltage Bank 2 Sensor 1 | DTC P0151, P0152, P0157, or P0158 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0153 | O2 Sensor Circuit Slow Response Bank 2 Sensor 1 | ECM | DTC P0133 or P0153 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
HO2S Slow Response Bank 2 Sensor 1 | DTC P0153, P0154, P0160, P1153, P2272, or P2273 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0154 | HO2S Circuit Insufficient Activity Bank 2 Sensor 1 | ECM | DTC P0134 or P0154 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
DTC P0153, P0154, P0160, P1153, P2272, or P2273 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0155 | O2 Sensor Heater Circuit Range/Performance Bank 2 Sensor 1 | ECM | DTC P0135, P0141, P0155, or P0161 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
HO2S Heater Performance Bank 2 Sensor 1 | DTC P0050, P0056, P0059, P0060, P0155, or P0161 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0157 | O2 Sensor Circuit Low Voltage Bank 2 Sensor 2 | ECM | DTC P0137, P0138, P0140, P0157, P0158, or P0160 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
HO2S Circuit Low Voltage Bank 2 Sensor 2 | DTC P0151, P0152, P0157, or P0158 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0158 | O2 Sensor Circuit High Voltage Bank 2 Sensor 2 | ECM | DTC P0137, P0138, P0140, P0157, P0158, or P0160 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
HO2S Circuit High Voltage Bank 2 Sensor 2 | DTC P0151, P0152, P0157, or P0158 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0160 | O2 Sensor Circuit No Activity Detected Bank 2 Sensor 2 | ECM | DTC P0137, P0138, P0140, P0157, P0158, or P0160 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
HO2S Circuit Insufficient Activity Bank 2 Sensor 2 | DTC P0153, P0154, P0160, P1153, P2272, or P2273 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0161 | O2 Sensor Heater Circuit Range/Performance Bank 2 Sensor 2 | ECM | DTC P0135, P0141, P0155, or P0161 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
HO2S Heater Performance Bank 2 Sensor 2 | ECM | DTC P0050, P0056, P0059, P0060, P0155, or P0161 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0171 | Fuel Trim System Lean Bank 1 | ECM | DTC P0171, P0172, P0174, or P0175
P0172 | Fuel Trim System Rich Bank 1 | ECM | DTC P0171, P0172, P0174, or P0175
P0174 | Fuel Trim System Lean Bank 2 | ECM | DTC P0171, P0172, P0174, or P0175
P0175 | Fuel Trim System Rich Bank 2 | ECM | DTC P0171, P0172, P0174, or P0175
P0196 | Engine Oil Temperature Sensor Range/Performance | ECM | DTC P0196, P0197, or P0198 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Engine Oil Temperature Sensor Circuit Range/Performance | ECM | DTC P0196, P0197, or P0198 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0197 | Engine Oil Temperature Voltage Low | ECM | DTC P0196, P0197, or P0198 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Engine Oil Temperature Sensor Circuit Low Input | ECM | DTC P0196, P0197, or P0198 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0198 | Engine Oil Temperature Voltage High | ECM | DTC P0196, P0197, or P0198 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Engine Oil Temperature Sensor Circuit High Input | ECM | DTC P0196, P0197, or P0198 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0201 | Injector 1 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0201, P0202, P0203, P0204, P0205, P0206, P0207, or P0208 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0202 | Injector 2 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0201, P0202, P0203, P0204, P0205, P0206, P0207, or P0208 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0203 | Injector 3 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0201, P0202, P0203, P0204, P0205, P0206, P0207, or P0208 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0204 | Injector 4 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0201, P0202, P0203, P0204, P0205, P0206, P0207, or P0208 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0205 | Injector 5 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0201, P0202, P0203, P0204, P0205, P0206, P0207, or P0208 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0206 | Injector 6 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0201, P0202, P0203, P0204, P0205, P0206, P0207, or P0208 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0207 | Injector 7 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0207, or P0208
P0208 | Injector 8 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0207, or P0208
P0218 | Transmission Fluid Overtemperature | TCM |

• | DTC P0218 for the 4L60-E/4L65-E/4L70-E transmission

• | DTC P0218 for the 5L40-E/5L50-E transmission

• | DTC P0218 for the 6L50/6L80/6L90 transmission

P0219 | Engine Overspeed Condition | ECM | DTC P0219
P0220 | Throttle Position Sensor 2 Circuit | ECM | DTC P0120, P0122, P0123, P0220, P0222, P0223, or P2135
P0221 | Throttle Position Sensor 2 Circuit Range/Performance | ECM | DTC P0121, P0122, P0123, P0221, P0222, or P0223
P0222 | Throttle Position Sensor 2 Circuit Low Voltage | ECM | DTC P0121, P0122, P0123, P0221, P0222, or P0223 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0120, P0122, P0123, P0220, P0222, P0223, or P2135 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0223 | Throttle Position Sensor 2 Circuit High Voltage | ECM | DTC P0121, P0122, P0123, P0221, P0222, or P0223 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0120, P0122, P0123, P0220, P0222, P0223, or P2135 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0230 | Fuel Pump Relay Control Circuit | ECM | DTC P0230
P0261 | Injector 1 Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0262 | Injector 1 Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0264 | Injector 2 Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0265 | Injector 2 Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0267 | Injector 3 Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0268 | Injector 3 Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0270 | Injector 4 Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0271 | Injector 4 Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0273 | Injector 5 Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0274 | Injector 5 Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0276 | Injector 6 Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0277 | Injector 6 Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0205, P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277
P0300 | Engine Misfire Detected | ECM | DTC P0300-P0306 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0300-P0308 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0301 | Cylinder 1 Misfire Detected | ECM | DTC P0300-P0306 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0300-P0308 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0302 | Cylinder 2 Misfire Detected | ECM | DTC P0300-P0306 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0300-P0308 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0303 | Cylinder 3 Misfire Detected | ECM | DTC P0300-P0306 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0300-P0308 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0304 | Cylinder 4 Misfire Detected | ECM | DTC P0300-P0306 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0300-P0308 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0305 | Cylinder 5 Misfire Detected | ECM | DTC P0300-P0306 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0300-P0308 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0306 | Cylinder 6 Misfire Detected | ECM | DTC P0300-P0306 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0300-P0308 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0307 | Cylinder 7 Misfire Detected | ECM | DTC P0300-P0308
P0308 | Cylinder 8 Misfire Detected | ECM | DTC P0300-P0308
P0315 | Crankshaft Position System Variation Not Learned | ECM | DTC P0315
P0324 | Knock Sensor Module Performance | ECM | DTC P0324 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0324, P0325, P0326, P0327, P0328, P0330, P0332, or P0333 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0325 | Knock Sensor (KS) Circuit Bank 1 | ECM | DTC P0324, P0325, P0326, P0327, P0328, P0330, P0332, or P0333
P0326 | Knock Sensor (KS) Performance Bank 1 | ECM | DTC P0326, P0327, P0328, P0331, P0332, or P0333 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Knock Sensor (KS) Performance | ECM | DTC P0324, P0325, P0326, P0327, P0328, P0330, P0332, or P0333 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0327 | Knock Sensor (KS) Circuit Low Voltage Bank 1 | ECM | DTC P0326, P0327, P0328, P0331, P0332, or P0333 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0324, P0325, P0326, P0327, P0328, P0330, P0332, or P0333 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0328 | Knock Sensor (KS) Circuit High Voltage Bank 1 | ECM | DTC P0326, P0327, P0328, P0331, P0332, or P0333 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0324, P0325, P0326, P0327, P0328, P0330, P0332, or P0333 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0330 | Knock Sensor (KS) Circuit Bank 2 | ECM | DTC P0324, P0325, P0326, P0327, P0328, P0330, P0332, or P0333
P0331 | Knock Sensor (KS) System Performance Bank 2 | ECM | DTC P0326, P0327, P0328, P0331, P0332, or P0333
P0332 | Knock Sensor (KS) Circuit Low Voltage Bank 2 | ECM | DTC P0326, P0327, P0328, P0331, P0332, or P0333 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0324, P0325, P0326, P0327, P0328, P0330, P0332, or P0333 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0333 | Knock Sensor (KS) Circuit High Voltage Bank 2 | ECM | DTC P0326, P0327, P0328, P0331, P0332, or P0333 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0324, P0325, P0326, P0327, P0328, P0330, P0332, or P0333 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0335 | Crankshaft Position Sensor Circuit Malfunction | ECM | DTC P0335, P0336, or P0338 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Crankshaft Position (CKP) Sensor Circuit | DTC P0335 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0336 | Crankshaft Position Sensor Signal Range/Performance | ECM | DTC P0335, P0336, or P0338 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Crankshaft Position (CKP) Sensor Performance | DTC P0336 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0338 | Crankshaft Position Sensor Circuit High Duty Cycle | ECM | DTC P0335, P0336, or P0338 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
P0340 | Camshaft Position (CMP) Sensor Circuit | ECM | DTC P0340
P0341 | Intake Camshaft Position Sensor Range/Performance Bank 1 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Camshaft Position (CMP) Sensor Performance | ECM | DTC P0341 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0342 | Intake Camshaft Position Sensor Low Voltage Bank 1 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0343 | Intake Camshaft Position Sensor High Voltage Bank 1 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0346 | Intake Camshaft Position Sensor Range/Performance Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0347 | Intake Camshaft Position Sensor Low Voltage Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0348 | Intake Camshaft Position Sensor High Voltage Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0350 | Ignition Coil Control Circuit | ECM | DTC P0350
P0351 | Ignition Coil Cylinder 1 Control Circuit | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0351-P0358 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0352 | Ignition Coil Cylinder 2 Control Circuit | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0351-P0358 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0353 | Ignition Coil Cylinder 3 Control Circuit | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0351-P0358 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0354 | Ignition Coil Cylinder 4 Control Circuit | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0351-P0358 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0355 | Ignition Coil Cylinder 5 Control Circuit | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0351-P0358 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0356 | Ignition Coil Cylinder 6 Control Circuit | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0351-P0358 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0357 | Ignition Coil Cylinder 7 Control Circuit | ECM | DTC P0351-P0358
P0358 | Ignition Coil Cylinder 8 Control Circuit | ECM | DTC P0351-P0358
P0366 | Exhaust Camshaft Position Sensor Range/Performance Bank 1 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0367 | Exhaust Camshaft Position Sensor Low Voltage Bank 1 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0368 | Exhaust Camshaft Position Sensor High Voltage Bank 1 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0391 | Exhaust Camshaft Position Sensor Range/Performance Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0392 | Exhaust Camshaft Position Sensor Low Voltage Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0393 | Exhaust Camshaft Position Sensor High Voltage Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0420 | Catalyst System Low EfficiencyBank 1 | ECM | DTC P0420 or P0430 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0420 or P0430 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0430 | Catalyst System Low Efficiency Bank 2 | ECM | DTC P0420 or P0430 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0420 or P0430 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0443 | Evaporative Emission Control System Purge Solenoid Circuit Malfunction | ECM | DTC P0443, P0458, or P0459 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0443 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0458 | Evaporative Emission Control System Purge Solenoid Circuit Low Voltage | ECM | DTC P0443, P0458, or P0459
P0459 | Evaporative Emission Control System Purge Solenoid Circuit High Voltage | ECM | DTC P0443, P0458, or P0459
P0461 | Fuel Level Sensor 1 Performance | ECM | DTC P0461
P0462 | Fuel Level Sensor 1 Circuit Low Voltage | ECM | DTC P0462
P0463 | Fuel Level Sensor 1 Circuit HighVoltage | ECM | DTC P0463
P0480 | Cooling Fan Relay 1 Control Circuit | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Cooling Fan 1 Control Circuit Malfunction | DTC P0480 or P0481 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0481 | Cooling Fan Relay 2 Control Circuit | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Cooling Fan 2 Control Circuit Malfunction | DTC P0480 or P0481 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0500 | Vehicle Speed Sensor Circuit Malfunction | ECM | DTC P0500
P0501 | Vehicle Speed Sensor (VSS) Performance | ECM | DTC P0501 or P0502
P0502 | Vehicle Speed Sensor (VSS) Circuit Low Voltage | ECM | DTC P0501 or P0502 for the Aisin AY6 transmission or DTC P0502 or P0503 for the Tremec 6-Speed transmission
P0503 | Vehicle Speed Sensor (VSS) Circuit Intermittent | ECM | DTC P0502 or P0503
P0506 | Idle Speed Low | ECM | DTC P0506, P0507, or P050A for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0506 or P0507 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0507 | Idle Speed High | ECM | DTC P0506, P0507, or P050A for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0506 or P0507 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P050A | Cold Start Idle Air Control (IAC) System Performance | ECM | DTC P0506, P0507, or P050A
P0521 | Engine Oil Pressure (EOP) Sensor Performance | ECM | DTC P0521, P0522, or P0523
P0522 | Engine Oil Pressure (EOP) Sensor Circuit Low Voltage | ECM | DTC P0521, P0522, or P0523
P0523 | Engine Oil Pressure (EOP) Sensor Circuit High Voltage | ECM | DTC P0521, P0522, or P0523
P0532 | Air Conditioning (A/C) Refrigerant Pressure Sensor Circuit | ECM | DTC P0532 or P0533
P0533 | Air Conditioning (A/C) Refrigerant Pressure Sensor Circuit Low Voltage | ECM | DTC P0532 or P0533
P0560 | System Voltage Malfunction | ECM | DTC P0560
P0562 | System Voltage Low | ECM | DTC P0562
TCM |

• | DTC P0562 or P0563 for the 4L60-E/4L65-E/4L70-E transmission

• | DTC P0562 or P0563 for the 5L40-E/5L50-E transmission

• | DTC P0562 or P0563 for the 6L50/6L80/6L90 transmission

P0563 | System Voltage High | ECM | DTC P0563
TCM |

• | DTC P0562 or P0563 for the 4L60-E/4L65-E/4L70-E transmission

• | DTC P0562 or P0563 for the 5L40-E/5L50-E transmission

• | DTC P0562 or P0563 for the 6L50/6L80/6L90 transmission

P0571 | Cruise Control Brake Switch Circuit | ECM | DTC P0571
P0575 | Cruise Control Enable Circuit Malfunction | ECM | DTC P0575
P0601 | Control Module Read Only Memory (ROM) Error | ECM | DTC P0601-P0604, P0606, P0607, P062B, P0167D, P2107, or P2610 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
Transmission Control Module (TCM) Read Only Memory (ROM) | TCM |

• | DTC P0601-P0604 or P062F for the 4L60-E/4L65-E/4L70-E transmission

• | DTC P0601-P0604 or P062F for the 5L40-E/5L50-E transmission

• | DTC P0601-P0604 or P062F for the 6L50/6L80/6L90 transmission

P0602 | Control Module Not Programmed | ECM | DTC P0601-P0604, P0606, P0607, P062B, P0167D, P2107, or P2610 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
Transmission Control Module (TCM) Not Programmed | TCM |

• | DTC P0601-P0604 or P062F for the 4L60-E/4L65-E/4L70-E transmission

• | DTC P0601-P0604 or P062F for the 5L40-E/5L50-E transmission

• | DTC P0601-P0604 or P062F for the 6L50/6L80/6L90 transmission

P0603 | Control Module Long Term Memory Reset | ECM | DTC P0601-P0604, P0606, P0607, P062B, P0167D, P2107, or P2610 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
Transmission Control Module (TCM) Long Term Memory Reset | TCM |

• | DTC P0601-P0604 or P062F for the 4L60-E/4L65-E/4L70-E transmission

• | DTC P0601-P0604 or P062F for the 5L40-E/5L50-E transmission

• | DTC P0601-P0604 or P062F for the 6L50/6L80/6L90 transmission

P0604 | Control Module Random Access Memory (RAM) | ECM | DTC P0601-P0604, P0606, P0607, P062B, P0167D, P2107, or P2610 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
Transmission Control Module (TCM) Random Access Memory (RAM) | TCM |

• | DTC P0601-P0604 or P062F for the 4L60-E/4L65-E/4L70-E transmission

• | DTC P0601-P0604 or P062F for the 5L40-E/5L50-E transmission

• | DTC P0601-P0604 or P062F for the 6L50/6L80/6L90 transmission

P0606 | Control Module Internal Performance | ECM | DTC P0601-P0604, P0606, P0607, P062B, P0167D, P2107, or P2610 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0607 | Control Module Performance | ECM | DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610
P060D | Control Module Accelerator Pedal Position (APP) System Performance | ECM | DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610
P0615 | Starter Relay Circuit Malfunction | ECM | DTC P0615
P0616 | Starter Relay Control Circuit Low Voltage | ECM | DTC P0616 or P0617
P0617 | Starter Relay Control Circuit High Voltage | ECM | DTC P0616 or P0617
P0621 | Alternator L-Terminal Circuit Malfunction | ECM | DTC P0621
P0622 | Generator F-Terminal Circuit | ECM | DTC P0622
P0625 | Generator F-Terminal Low Voltage | ECM | DTC P0625 or P0626
P0626 | Generator F-Terminal High Voltage | ECM | DTC P0625 or P0626
P0627 | Fuel Pump Relay Control Circuit | ECM | DTC P0627, P0628, or P0629
P0628 | Fuel Pump Relay Control Circuit Low Voltage | ECM | DTC P0627, P0628, or P0629
P0629 | Fuel Pump Relay Control Circuit High Voltage | ECM | DTC P0627, P0628, or P0629
P062F | Control Module Long Term Memory Performance | ECM | DTC P0601-P0604, P0606, P0607, P062B, P0167D, P2107, or P2610 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
Transmission Control Module (TCM) Long Term Memory Performance | TCM |

• | DTC P0601-P0604 or P062F for the 4L60-E/4L65-E/4L70-E transmission

• | DTC P0601-P0604 or P062F for the 5L40-E/5L50-E transmission

• | DTC P0601-P0604 or P062F for the 6L50/6L80/6L90 transmission

P0633 | Theft Deterrent Key Not Programmed | ECM | DTC P0633
P0634 | Transmission Control Module (TCM) Overtemperature | TCM | DTC P0634
P0638 | Commanded versus Actual Throttle Position Correlation | ECM | DTC P0638, P2100, P2101, or P2119
P0641 | 5-Volt Reference 1 Circuit | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
5V Reference Circuit 1 Malfunction | DTC P0641 or P0651 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0642 | 5-Volt Reference 1 Circuit Low Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P0643 | 5-Volt Reference 1 Circuit High Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P0650 | Malfunction Indicator (MI) Circuit Malfunction | ECM | DTC P0650 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0650 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0651 | 5-Volt Reference 2 Circuit | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
5V Reference Circuit 2 Malfunction | ECM | DTC P0641 or P0651 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0652 | 5-Volt Reference 2 Circuit Low Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P0653 | 5-Volt Reference 2 Circuit High Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P0660 | Intake Manifold Tuning (IMT) Valve Solenoid Control Circuit | ECM | DTC P0660, P0661, or P0662
P0661 | Intake Manifold Tuning (IMT) Solenoid Control Circuit Low Voltage | ECM | DTC P0660, P0661, or P0662
P0662 | Intake Manifold Tuning (IMT) Solenoid Control Circuit High Voltage | ECM | DTC P0660, P0661, or P0662
P0667 | Transmission Control Module (TCM) Temperature Sensor Performance | TCM | DTC P0667, P0668, or P0669
P0668 | Transmission Control Module (TCM) Temperature Sensor Circuit Low Voltage | TCM | DTC P0667, P0668, or P0669
P0669 | Transmission Control Module (TCM) Temperature Sensor Circuit High Voltage | TCM | DTC P0667, P0668, or P0669
P0685 | Engine Control Ignition Relay Circuit Malfunction | ECM | DTC P0685, P0686, P0687, P0689, or P0690 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Engine Controls Ignition Relay Control Circuit | ECM | DTC P0685, P0689, or P0690 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0686 | Engine Control Ignition Relay Circuit Low Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690
P0687 | Engine Control Ignition Relay Circuit High Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690
P0689 | Engine Control Ignition Relay Feedback Circuit Low Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Engine Controls Relay Feedback Circuit Low Voltage | DTC P0685, P0689, or P0690 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0690 | Engine Control Ignition Relay Feedback Circuit High Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Engine Controls Relay Feedback Circuit High Voltage | DTC P0685, P0689, or P0690 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0691 | Cooling Fan Relay 1 Control Circuit Low Voltage | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694
P0692 | Cooling Fan Relay 2 Control Circuit High Voltage | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694
P0693 | Cooling Fan Relay 2 Control Circuit Low Voltage | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694
P0694 | Cooling Fan Relay 1 Control Circuit High Voltage | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694
P0697 | 5-Volt Reference 3 Circuit | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P0698 | 5-Volt Reference 3 Circuit Low Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P0699 | 5-Volt Reference 3 Circuit High Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P0700 | Transmission Control Module (TCM) Requested MIL Illumination | ECM | DTC P0700 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0700 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P0703 | Torque Converter / Brake Switch Circuit Malfunction | ECM | DTC P0703
P0704 | Clutch Switch Circuit | ECM | DTC P0704
P0705 | Transmission Range (TR) Switch Circuit | TCM | DTC P0705
P0711 | Transmission Fluid Temperature (TFT) Sensor Performance | TCM |

• | DTC P0711 for the 4L60-E/4L65-E/4L70-E transmission

• | DTC P0711 for the 5L40-E/5L50-E transmission

• | DTC P0711, P0712, or P0713 for the 6L50/6L80/6L90 transmission

P0712 | Transmission Fluid Temperature (TFT) Sensor Circuit Low Voltage | ECM | DTC P0712 or P0713 for the Tremec 6-Speed transmission
TCM |

• | DTC P0712 or P0713 for the 4L60-E/4L65-E/4L70-E transmission

• | DTC P0712 or P0713 for the 5L40-E/5L50-E transmission

• | DTC P0711, P0712, or P0713 for the 6L50/6L80/6L90 transmission

P0713 | Transmission Fluid Temperature (TFT) Sensor Circuit High Voltage | ECM | DTC P0712 or P0713 for the Tremec 6-Speed transmission
TCM |

• | DTC P0712 or P0713 for the 4L60-E/4L65-E/4L70-E transmission

• | DTC P0712 or P0713 for the 5L40-E/5L50-E transmission

• | DTC P0711, P0712, or P0713 for the 6L50/6L80/6L90 transmission

P0716 | Input Speed Sensor Performance | TCM |

• | DTC P0716 or P0717 for the 4L60-E/4L65-E/4L70-E transmission

• | DTC P0716 or P0717 for the 5L40-E/5L50-E transmission

• | DTC P0716 or P0717 for the 6L50/6L80/6L90 transmission

P0717 | Input Speed Sensor Circuit Low Voltage | TCM |

• | DTC P0716 or P0717 for the 4L60-E/4L65-E/4L70-E transmission

• | DTC P0716 or P0717 for the 5L40-E/5L50-E transmission

• | DTC P0716 or P0717 for the 6L50/6L80/6L90 transmission

P0719 | Brake Switch Circuit Low Voltage | TCM | DTC P0719 or P0724
P071A | Transmission Tow Mode Switch Circuit | TCM | DTC P071A
P0722 | Output Speed Sensor Circuit Low Voltage | TCM |

• | DTC P0722 or P0723 for the 4L60-E/4L65-E/4L70-E transmission

• | DTC P0722 or P0723 for the 5L40-E/5L50-E transmission

• | DTC P0722 or P0723 for the 6L50/6L80/6L90 transmission

P0723 | Output Speed Sensor Circuit Intermittent | TCM |

• | DTC P0722 or P0723 for the 4L60-E/4L65-E/4L70-E transmission

• | DTC P0722 or P0723 for the 5L40-E/5L50-E transmission

• | DTC P0722 or P0723 for the 6L50/6L80/6L90 transmission

P0724 | Brake Switch Circuit High Voltage | TCM | DTC P0719 or P0724
P0741 | Torque Converter Clutch (TCC) System - Stuck Off | TCM |

• | DTC P0741, P0751, or P0756 for the 4L60-E/4L65-E/4L70-E transmission

• | DTC P0741, P0751, P0756, or P0761 for the 5L40-E/5L50-E transmission

• | DTC P0741 or P0742 for the 6L50/6L80/6L90 transmission

P0742 | Torque Converter Clutch (TCC) System - Stuck On | TCM |

• | DTC P0742, P0752, or P0757 for the 4L60-E/4L65-E/4L70-E transmission

• | DTC P0742, P0752, P0757, or P0762 for the 5L40-E/5L50-E transmission

• | DTC P0741 or P0742 for the 6L50/6L80/6L90 transmission

P0748 | Pressure Control (PC) Solenoid Control Circuit | TCM | DTC P0748
P0751 | 1-2 Shift Solenoid (SS) Valve Performance - No First, Fourth or Fifth Gear | TCM | DTC P0741, P0751, or P0756 for the 4L60-E/4L65-E/4L70-E transmission or DTC P0741, P0751, P0756, or P0761 for the 5L40-E/5L50-E transmission
Shift Solenoid (SS) 1 Valve Performance - Stuck Off | DTC P0751 for the 6L50/6L80/6L90 transmission
P0752 | 1-2 Shift Solenoid (SS) Valve Performance - No Second or Third Gear | TCM | DTC P0742, P0752, or P0757 for the 4L60-E/4L65-E/4L70-E transmission or DTC P0742, P0752, P0757, or P0762 for the 5L40-E/5L50-E transmission
Shift Solenoid (SS) 1 Valve Performance - Stuck On | DTC P0752 for the 6L50/6L80/6L90 transmission
P0756 | 2-3 Shift Solenoid (SS) Valve Performance - No First or Second Gear | TCM | DTC P0741, P0751, or P0756 for the 4L60-E/4L65-E/4L70-E transmission or DTC P0741, P0751, P0756, or P0761 for the 5L40-E/5L50-E transmission
Shift Solenoid (SS) 2 Valve Performance - Stuck Off | DTC P0756 for the 6L50/6L80/6L90 transmission
P0757 | 2-3 Shift Solenoid (SS) Valve Performance - No Third, Fourth or Fifth Gear | TCM | DTC P0742, P0752, or P0757 for the 4L60-E/4L65-E/4L70-E transmission or DTC P0742, P0752, P0757, or P0762 for the 5L40-E/5L50-E transmission
P0761 | 4-5 Shift Solenoid (SS) Valve Performance - No Fourth Gear | TCM | DTC P0741, P0751, P0756, or P0761
P0762 | 4-5 Shift Solenoid (SS) Valve Performance - No Fifth Gear | TCM | DTC P0742, P0752, P0757, or P0762
P0776 | Clutch Pressure Control (PC) Solenoid 2 - Stuck Off | TCM | DTC P0776 or P0777
P0777 | Clutch Pressure Control (PC) Solenoid 2 - Stuck On | TCM | DTC P0776 or P0777
P0787 | 3-2 Shift Solenoid (SS) Control Circuit Low Voltage | TCM | DTC P0787 or P0788
P0788 | 3-2 Shift Solenoid (SS) Control Circuit High Voltage | TCM | DTC P0787 or P0788
P0796 | Clutch Pressure Control (PC) Solenoid 3 - Stuck Off | TCM | DTC P0796 or P0797
P0797 | Clutch Pressure Control (PC) Solenoid 3 - Stuck On | TCM | DTC P0796 or P0797
P0801 | Reverse Lockout Solenoid Control Circuit | ECM | DTC P0801
P0803 | Skip Shift Solenoid Control Circuit | ECM | DTC P0803
P0806 | Clutch Pedal Position (CPP) Sensor Circuit Performance | ECM | DTC P0806 for the Aisin AY6 transmission or DTC P0806 for the Tremec 6-Speed transmission
P0807 | Clutch Pedal Position (CPP) Sensor Circuit Low Voltage | ECM | DTC P0807 or P0808 for the Aisin AY6 transmission or DTC P0807 or P0808 for the Tremec 6-Speed transmission
P0808 | Clutch Pedal Position (CPP) Sensor Circuit High Voltage | ECM | DTC P0807 or P0808 for the Aisin AY6 transmission or DTC P0807 or P0808 for the Tremec 6-Speed transmission
P080A | Clutch Pedal Position (CPP) Sensor Circuit High Voltage | ECM | DTC P080A for the Aisin AY6 transmission or DTC P080A for the Tremec 6-Speed transmission
P0815 | Upshift Switch Circuit | TCM | DTC P0815 or P816 for the 5L40-E/5L50-E transmission or DTC P0815, P0816, or P0826 for the 6L50/6L80/6L90 transmission
P0816 | Downshift Switch Circuit | TCM | DTC P0815 or P816 for the 5L40-E/5L50-E transmission or DTC P0815, P0816, or P0826 for the 6L50/6L80/6L90 transmission
P0826 | Up and Down Shift Switch Circuit | TCM | DTC P0115, P0120, P0826, P2544, or P2637 for the 5L40-E/5L50-E transmission or DTC P0815, P0816, or P0826 for the 6L50/6L80/6L90 transmission
P0842 | Transmission Fluid Pressure (TFP) Switch 1 Circuit Low Voltage | TCM | DTC P0842 or P0843
P0843 | Transmission Fluid Pressure (TFP) Switch 1 Circuit High Voltage | TCM | DTC P0842 or P0843
P0850 | Park/Neutral Position (PNP) Switch Circuit | TCM | DTC P0850
P0851 | Park/Neutral Position (PNP) Switch Circuit Low Voltage | ECM | DTC P0851 or P0852 for the 4L60-E/4L65-E/4L70-E transmission or DTC P0851 or P0852 for the 6L50/6L80/6L90 transmission
P0852 | Park/Neutral Position (PNP) Switch Circuit High Voltage | ECM | DTC P0851 or P0852 for the 4L60-E/4L65-E/4L70-E transmission or DTC P0851 or P0852 for the 6L50/6L80/6L90 transmission
P0856 | Engine Control Module (ECM) Traction Control Torque Request Circuit | ECM | DTC P0856
P0872 | Transmission Fluid Pressure (TFP) Switch 3 Circuit Low Voltage | TCM | DTC P0872 or P0873
P0873 | Transmission Fluid Pressure (TFP) Switch 3 Circuit High Voltage | TCM | DTC P0872 or P0873
P0877 | Transmission Fluid Pressure (TFP) Switch 4 Circuit Low Voltage | TCM | DTC P0877 or P0878
P0878 | Transmission Fluid Pressure (TFP) Switch 4 Circuit High Voltage | TCM | DTC P0877 or P0878
P0897 | Transmission Fluid Life | TCM | DTC P0897
P0961 | Line Pressure Control (PC) Solenoid System Performance | TCM | DTC P0961 for the 4L60-E/4L65-E/4L70-E transmission or DTC P0961-P0963 for the 6L50/6L80/6L90 transmission
P0962 | Line Pressure Control (PC) Solenoid Control Circuit Low Voltage | TCM | DTC P0961-P0963
P0963 | Line Pressure Control (PC) Solenoid Control Circuit High Voltage | TCM | DTC P0961-P0963
P0965 | Clutch Pressure Control (PC) Solenoid 2 System Performance | TCM | DTC P0965-P0967
P0966 | Clutch Pressure Control (PC) Solenoid 2 Control Circuit Low Voltage | TCM | DTC P0965-P0967
P0967 | Clutch Pressure Control (PC) Solenoid 2 Control Circuit High Voltage | TCM | DTC P0965-P0967
P0969 | Clutch Pressure Control (PC) Solenoid 3 System Performance | TCM | DTC P0969-P0971
P0970 | Clutch Pressure Control (PC) Solenoid 3 Control Circuit Low Voltage | TCM | DTC P0969-P0971
P0971 | Clutch Pressure Control (PC) Solenoid 3 Control Circuit High Voltage | TCM | DTC P0969-P0971
P0973 | 1-2 Shift Solenoid (SS) Control Circuit Low Voltage | TCM | DTC P0973, P0976, or P2764 for the 4L60-E/4L65-E/4L70-E transmission or DTC P0973, P0976, P0979, or P2764 for the 5L40-E/5L50-E transmission
Shift Solenoid (SS) 1 Control Circuit Low Voltage | DTC P0973 or P0974 for the 6L50/6L80/6L90 transmission
P0974 | 1-2 Shift Solenoid (SS) Control Circuit High Voltage | TCM | DTC P0974, P0977, or P2763 for the 4L60-E/4L65-E/4L70-E transmission or DTC P0974, P0977, P0980, or P2763 for the 5L40-E/5L50-E transmission
Shift Solenoid (SS) 1 Control Circuit High Voltage | DTC P0973 or P0974 for the 6L50/6L80/6L90 transmission
P0976 | 2-3 Shift Solenoid (SS) Control Circuit Low Voltage | TCM | DTC P0973, P0976, or P2764 for the 4L60-E/4L65-E/4L70-E transmission or DTC P0973, P0976, P0979, or P2764 for the 5L40-E/5L50-E transmission
Shift Solenoid (SS) 2 Control Circuit Low Voltage | DTC P0976 or P0977 for the 6L50/6L80/6L90 transmission
P0977 | 2-3 Shift Solenoid (SS) Control Circuit High Voltage | TCM | DTC P0974, P0977, or P2763 for the 4L60-E/4L65-E/4L70-E transmission or DTC P0974, P0977, P0980, or P2763 for the 5L40-E/5L50-E transmission
Shift Solenoid (SS) 2 Control Circuit High Voltage | DTC P0976 or P0977 for the 6L50/6L80/6L90 transmission
P0979 | 4-5 Shift Solenoid (SS) Control Circuit Low Voltage | TCM | DTC P0973, P0976, P0979, or P2764
P0980 | 4-5 Shift Solenoid (SS) Control Circuit High Voltage | TCM | DTC P0974, P0977, P0980, or P2763
P0989 | Transmission Fluid Pressure (TFP) Switch 5 Circuit Low Voltage | TCM | DTC P0989 or P0990
P0990 | Transmission Fluid Pressure (TFP) Switch 5 Circuit High Voltage | TCM | DTC P0989 or P0990
P1011 | Intake Camshaft Actuator Park Position Bank 1 | ECM | DTC P1011-P1014
P1012 | Exhaust Camshaft Actuator Park Position Bank 1 | ECM | DTC P1011-P1014
P1013 | Intake Camshaft Actuator Park Position Bank 2 | ECM | DTC P1011-P1014
P1014 | Exhaust Camshaft Actuator Park Position Bank 2 | ECM | DTC P1011-P1014
P1101 | Intake Air Flow System Performance | ECM | DTC P0101 or P1101
P1133 | HO2S Insufficient Switching Bank 1 Sensor 1 | ECM | DTC P0133, P0134, P0140, P1133, P2270, or P2271
P1153 | HO2S Insufficient Switching Bank 2 Sensor 1 | ECM | DTC P0153, P0154, P0160, P1153, P2272, or P2273
P1174 | Fuel Trim Cylinder Balance Bank 1 | ECM | DTC P1174 or P1175
P1175 | Fuel Trim Cylinder Balance Bank 2 | ECM | DTC P1174 or P1175
P1258 | Engine Coolant Over Temperature - Protection Mode Active | ECM | DTC P1258
P1380 | Misfire Detected - Rough Road Data Not Available | ECM | DTC P1380 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P1380 or P1381 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P1381 | Misfire Detected - No Communication with Brake Control Module | ECM | DTC P1380 or P1381
P1400 | Cold Start Emission Reduction Control System | ECM | DTC P1400
P150A | Transmission Output Speed Signal Circuit | TCM | DTC P150A or P150B
P150B | Transmission Output Speed Sensor Circuit Intermittent | TCM | DTC P150A or P150B
P1516 | Throttle Actuator Control (TAC) Module Throttle Actuator Position Performance | ECM | DTC P1516, P2101, P2119, or P2176
P1551 | Throttle Control Lower Position not Reached during Learning Mode | ECM | DTC P1551
P1631 | Theft Deterrent Fuel Enable Signal Not Correct | ECM | DTC P1631
P1668 | Generator L-Terminal Control Circuit | ECM | DTC P1668, P2500, or P2501
P167D | Control Module Ignition Coil Internal Circuit | ECM | DTC P0601-P0604, P0606, P0607, P062B, P0167D, P2107, or P2610
P1682 | Ignition 1 Switch Circuit 2 | ECM | DTC P1682
P1684 | Transmission Control Module (TCM) Power Up Temperature Sensor Performance | TCM | DTC P1684-P1686
P1685 | Transmission Control Module (TCM) Power Up Temperature Sensor Circuit Low Voltage | TCM | DTC P1684-P1686
P1686 | Transmission Control Module (TCM) Power Up Temperature Sensor Circuit High Voltage | TCM | DTC P1684-P1686
P1751 | Shift Valve 1 Performance | TCM | DTC P1751
P1761 | Up and Down Shift Switch Signal Circuit | TCM | DTC P1761
P1762 | Transmission Mode Switch Signal Circuit | TCM | DTC P1762 for the 4L60-E/4L65-E/4L70-E transmission or DTC P1762 for the 5L40-E/5L50-E transmission
P1810 | Transmission Fluid Pressure (TFP) Position Switch Circuit | TCM | DTC P1810, P1815, P1816, or P1818
P1815 | Transmission Fluid Pressure (TFP) Valve Position Switch - Start in Wrong Range | TCM | DTC P1810, P1815, P1816, or P1818
P1816 | Transmission Fluid Pressure (TFP) Valve Position Switch Indicates Park/Neutral (P/N) with Drive Ratio | TCM | DTC P1810, P1815, P1816, or P1818
P1818 | Transmission Fluid Pressure (TFP) Valve Position Switch Indicates Drive without Drive Ratio | TCM | DTC P1810, P1815, P1816, or P1818
P1820 | Internal Mode Switch A Circuit Low Voltage | TCM | DTC P1820, P1822, P1823, P1825, P1826, or P1915
P1822 | Internal Mode Switch B Circuit High Voltage | TCM | DTC P1820, P1822, P1823, P1825, P1826, or P1915
P1823 | Internal Mode Switch P Circuit Low Voltage | TCM | DTC P1820, P1822, P1823, P1825, P1826, or P1915
P1825 | Internal Mode Switch - Invalid Range | TCM | DTC P1820, P1822, P1823, P1825, P1826, or P1915 for the 5L40-E/5L50-E transmission or DTC P1825 or P1915 for the 6L50/6L80/6L90 transmission
P1826 | Internal Mode Switch C Circuit High Voltage | TCM | DTC P1820, P1822, P1823, P1825, P1826, or P1915
P1831 | Pressure Control (PC)/Shift Lock Solenoid Control Circuit Low Voltage | TCM | DTC P1831 or P1832 for the 5L40-E/5L50-E transmission or DTC P1831 or P1832 for the 6L50/6L80/6L90 transmission
P1832 | Pressure Control (PC)/Shift Lock Solenoid Control Circuit High Voltage | TCM | DTC P1831 or P1832 for the 5L40-E/5L50-E transmission or DTC P1831 or P1832 for the 6L50/6L80/6L90 transmission
P1833 | Torque Converter Clutch (TCC)/Shift Solenoid (SS) Control Circuit Low Voltage | TCM | DTC P1833 or P1834
P1834 | Torque Converter Clutch (TCC)/Shift Solenoid (SS) Control Circuit High Voltage | TCM | DTC P1833 or P1834
P1876 | Up and Down Shift Switch Performance - Range Switch Not in D3 | TCM | DTC P1876 for the 5L40-E/5L50-E transmission or DTC P1876 for the 6L50/6L80/6L90 transmission
P1915 | Internal Mode Switch Does Not Indicate Park/Neutral (P/N) During Start | TCM | DTC P1820, P1822, P1823, P1825, P1826, or P1915 for the 5L40-E/5L50-E transmission
Internal Mode Switch Start/Wrong Range | DTC P1825 or P1915 for the 6L50/6L80/6L90 transmission
P2008 | Intake Manifold Runner Control Solenoid Circuit Malfunction | ECM | DTC P2008, P2009, or P2010
P2009 | Intake Manifold Runner Control Solenoid Circuit Low Voltage | ECM | DTC P2008, P2009, or P2010
P2010 | Intake Manifold Runner Control Solenoid Circuit High Voltage | ECM | DTC P2008, P2009, or P2010
P2066 | Fuel Level Sensor 2 Performance | ECM | DTC P2066
P2067 | Fuel Level Sensor 2 Low Voltage | ECM | DTC P2067
P2068 | Fuel Level Sensor 2 High Voltage | ECM | DTC P2068
P2072 | Throttle Actuator Control System - Ice Blockage | ECM | DTC P2072
P2076 | Intake Manifold Runner Control (IMRC) Solenoid Performance | ECM | DTC P2076, P2077, or P2078
P2077 | Intake Manifold Runner Control (IMRC) Solenoid Circuit Low Voltage | ECM | DTC P2076, P2077, or P2078
P2078 | Intake Manifold Runner Control (IMRC) Solenoid Circuit High Voltage | ECM | DTC P2076, P2077, or P2078
P2088 | Intake Camshaft Position Control Solenoid Circuit Low Voltage Bank 1 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2089 | Intake Camshaft Position Control Solenoid Circuit High Voltage Bank 1 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2090 | Exhaust Camshaft Position Control Solenoid Circuit Low Voltage Bank 1 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2091 | Exhaust Camshaft Position Control Solenoid Circuit High Voltage Bank 1 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2092 | Intake Camshaft Position Control Solenoid Circuit Low Voltage Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2093 | Intake Camshaft Position Control Solenoid Circuit High Voltage Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2094 | Exhaust Camshaft Position Control Solenoid Circuit Low Voltage Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2095 | Exhaust Camshaft Position Control Solenoid Circuit High Voltage Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P2096 | Post Catalyst O2 Sensor Fuel Trim Below Lower Limit Bank 1 | ECM | DTC P2096 or P2098
P2097 | Post Catalyst O2 Sensor Fuel Trim Above Upper Limit Bank 1 | ECM | DTC P2097 or P2099
P2098 | Post Catalyst O2 Sensor Fuel Trim Below Lower Limit Bank 2 | ECM | DTC P2096 or P2098
P2099 | Post Catalyst O2 Sensor Fuel Trim Above Upper Limit Bank 2 | ECM | DTC P2097 or P2099
P2100 | Throttle Control Motor Malfunction | ECM | DTC P0638, P2100, P2101, or P2119
P2101 | Throttle Control Position Range/Performance | ECM | DTC P0638, P2100, P2101, or P2119 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Throttle Actuator Position Performance | DTC P1516, P2101, P2119, or P2176 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P2105 | Throttle Control Forced Engine Shutdown | ECM | DTC P2105
P2119 | Closed Throttle Position Range/Performance | ECM | DTC P0638, P2100, P2101, or P2119 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Throttle Closed Position Performance | DTC P1516, P2101, P2119, or P2176 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P2120 | Accelerator Pedal Position Sensor 1 Circuit | ECM | DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138
P2122 | Accelerator Pedal Position Sensor 1 Low Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P2123 | Accelerator Pedal Position Sensor 1 High Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P2125 | Accelerator Pedal Position Sensor 2 Circuit | ECM | DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138
P2127 | Accelerator Pedal Position Sensor 2Low Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P2128 | Accelerator Pedal Position Sensor 2 High Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P2135 | Throttle Position Sensor 1-2 Correlation | ECM | DTC P0120, P0122, P0123, P0220, P0222, P0223, or P2135
P2138 | Accelerator Pedal Position Sensor 1-2 Correlation | ECM | DTC P2122, P2123, P2127, P2128, or P2138 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P2176 | Throttle Actuator Control Lower Position Not Learned | ECM | DTC P2176 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
Minimum Throttle Position Not Learned | DTC P1516, P2101, P2119, or P2176 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P2177 | Fuel Trim Lean during Cruising/Acceleration Bank 1 | ECM | DTC P2177, P2179, P2187, or P2189
P2178 | Fuel Trim Rich during Cruising/Acceleration Bank 1 | ECM | DTC P2178, P2180, P2188, or P2190
P2179 | Fuel Trim Lean during Cruising/Acceleration Bank 2 | ECM | DTC P2177, P2179, P2187, or P2189
P2180 | Fuel Trim Rich during Cruising/Acceleration Bank 2 | ECM | DTC P2178, P2180, P2188, or P2190
P2187 | Fuel Trim Lean during Idling/Deceleration Bank 1 | ECM | DTC P2177, P2179, P2187, or P2189
P2188 | Fuel Trim Rich during Idling/Deceleration Bank 1 | ECM | DTC P2178, P2180, P2188, or P2190
P2189 | Fuel Trim Lean during Idling/Deceleration Bank 2 | ECM | DTC P2177, P2179, P2187, or P2189
P2190 | Fuel Trim Rich during Idling/Deceleration Bank 2 | ECM | DTC P2178, P2180, P2188, or P2190
P2227 | Barometric Pressure Sensor Range/Performance | ECM | DTC P2227, P2228, or P2229
P2228 | Barometric Pressure Sensor Voltage Low | ECM | DTC P2227, P2228, or P2229
P2229 | Barometric Pressure Sensor Voltage High | ECM | DTC P2227, P2228, or P2229
P2231 | HO2S Signal Circuit Shorted to Heater Circuit Bank 1 Sensor 1 | ECM | DTC P2231, P2232, P2234, or P2235
P2232 | HO2S Signal Circuit Shorted to Heater Circuit Bank 1 Sensor 2 | ECM | DTC P2232 or P2235 or DTC P2231, P2232, P2234, or P2235
P2234 | HO2S Signal Circuit Shorted to Heater Circuit Bank 2 Sensor 1 | ECM | DTC P2231, P2232, P2234, or P2235
P2235 | HO2S Signal Circuit Shorted to Heater Circuit Bank 2 Sensor 2 | ECM | DTC P2232 or P2235 or DTC P2231, P2232, P2234, or P2235
P2237 | HO2S Pumping Current Control Circuit Bank 1 Sensor 1 | ECM | DTC P2237-P2242
P2239 | O2 Sensor Pump Current Circuit Low Voltage Bank 1 Sensor 1 | ECM | DTC P2237-P2242
P2240 | HO2S Pumping Current Control Circuit Bank 2 Sensor 1 | ECM | DTC P2237-P2242
P2242 | O2 Sensor Pump Current Circuit High Voltage Bank 2 Sensor 1 | ECM | DTC P2237-P2242
P2243 | HO2S Reference Voltage Circuit Bank 1 Sensor 1 | ECM | DTC P2243 or P2247
P2247 | HO2S Reference Voltage Circuit Bank 2 Sensor 1 | ECM | DTC P2243 or P2247
P2251 | HO2S Reference Ground Circuit Bank 1 Sensor 1 | ECM | DTC P2251 or P2254
P2254 | HO2S Reference Ground Circuit Bank 2 Sensor 1 | ECM | DTC P2251 or P2254
P2270 | O2 Sensor Lean/Rich Switch Signal Malfunction Bank 1 Sensor 2 | ECM | DTC P2270 or P2272 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
HO2S Signal Stuck Lean Bank 1 Sensor 2 | DTC P0133, P0134, P0140, P1133, P2270, or P2271 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P2271 | O2 Sensor Rich/Lean Switch Signal Malfunction Bank 1 Sensor 2 | ECM | DTC P2271 or P2273 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
HO2S Signal Stuck Rich Bank 1 Sensor 2 | DTC P0133, P0134, P0140, P1133, P2270, or P2271 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P2272 | O2 Sensor Lean/Rich Switch Signal Malfunction Bank 2 Sensor 2 | ECM | DTC P2270 or P2272 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
HO2S Signal Stuck Lean Bank 2 Sensor 2 | DTC P0153, P0154, P0160, P1153, P2272, or P2273 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P2273 | O2 Sensor Rich/Lean Switch Signal Malfunction Bank 2 Sensor 2 | ECM | DTC P2271 or P2273 for the 2.8L, 3.0L, 3.2L, or 3.6L engine
HO2S Signal Stuck Rich Bank 2 Sensor 2 | DTC P0153, P0154, P0160, P1153, P2272, or P2273 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P2297 | HO2S Performance During Decel Fuel Cut-Off Bank 1 Sensor 1 | ECM | DTC P2297 or P2298
P2298 | HO2S Performance During Decel Fuel Cut-Off Bank 2 Sensor 1 | ECM | DTC P2297 or P2298
P2300 | Ignition Coil Cylinder 1 Circuit Low Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2301 | Ignition Coil Cylinder 1 Circuit High Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2303 | Ignition Coil Cylinder 2 Circuit Low Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2304 | Ignition Coil Cylinder 2 Circuit High Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2306 | Ignition Coil Cylinder 3 Circuit Low Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2307 | Ignition Coil Cylinder 3 Circuit High Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2309 | Ignition Coil Cylinder 4 Circuit Low Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2310 | Ignition Coil Cylinder 4 Circuit High Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2312 | Ignition Coil Cylinder 5 Circuit Low Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2313 | Ignition Coil Cylinder 5 Circuit High Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2315 | Ignition Coil Cylinder 6 Circuit Low Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2316 | Ignition Coil Cylinder 6 Circuit High Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P250A | Engine Oil Level Sensor Circuit | ECM | DTC P250A
P2500 | Generator L-Terminal Circuit Low Voltage | ECM | DTC P1668, P2500, or P2501
P2501 | Generator L-Terminal Circuit High Voltage | ECM | DTC P1668, P2500, or P2501
P2534 | Ignition 1 Switch Circuit Low Voltage | TCM |

• | DTC P2534 for the 4L60-E/4L65-E/4L70-E transmission

• | DTC P2534 for the 5L40-E/5L50-E transmission

• | DTC P2534 for the 6L50/6L80/6L90 transmission

P2544 | Transmission Torque Request Circuit | ECM | DTC P2544 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
TCM | DTC P0115, P0120, P0826, P2544, or P2637 for the 5L40-E/5L50-E transmission
P2610 | Control Module Ignition Off Timer Performance | ECM | DTC P0601-P0604, P0606, P0607, P062B, P0167D, P2107, or P2610 for the 2.8L, 3.0L, 3.2L, or 3.6L engine or DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 4.8L, 5.3L, 6.0L, 6.2L, or 7.0L engine
P2636 | Fuel Transfer Pump Flow Insufficient | ECM | DTC P0656 or P2636
P2637 | Transmission Torque Delivered Circuit | TCM | DTC P0115, P0120, P0826, P2544, or P2637
P2714 | Clutch Pressure Control (PC) Solenoid 4 - Stuck Off | TCM | DTC P2714 or P2715
P2715 | Clutch Pressure Control (PC) Solenoid?4 - Stuck On | TCM | DTC P2714 or P2715
P2719 | Clutch Pressure Control (PC) Solenoid 4 System Performance | TCM | DTC P2719-P2721
P2720 | Clutch Pressure Control (PC) Solenoid 4 Control Circuit Low Voltage | TCM | DTC P2719-P2721
P2721 | Clutch Pressure Control (PC) Solenoid 4 Control Circuit High Voltage | TCM | DTC P2719-P2721
P2723 | Clutch Pressure Control (PC) Solenoid 5 - Stuck Off | TCM | DTC P2723 or P2724
P2724 | Clutch Pressure Control (PC) Solenoid 5 - Stuck On | TCM | DTC P2723 or P2724
P2728 | Clutch Pressure Control (PC) Solenoid 5 System Performance | TCM | DTC P2728-P2730
P2729 | Clutch Pressure Control (PC) Solenoid 5 Control Circuit Low Voltage | TCM | DTC P2728-P2730
P2730 | Clutch Pressure Control (PC) Solenoid 5 Control Circuit High Voltage | TCM | DTC P2728-P2730
P2762 | Torque Converter Clutch (TCC) Pressure Control Solenoid System Performance | TCM | DTC P2762, P2763, or P2764
P2763 | Torque Converter Clutch (TCC) Pressure Control (PC) Solenoid Control Circuit High Voltage | TCM | DTC P0974, P0977, or P2763 for the 4L60-E/4L65-E/4L70-E transmission or DTC P0974, P0977, P0980, or P2763 for the 5L40-E/5L50-E transmission
Torque Converter Clutch (TCC) Pressure Control Solenoid Control Circuit Low Voltage | DTC P2762, P2763, or P2764 for the 6L50/6L80/6L90 transmission
P2764 | Torque Converter Clutch (TCC) Pressure Control (PC) Solenoid Control Circuit Low Voltage | TCM | DTC P0973, P0976, or P2764 for the 4L60-E/4L65-E/4L70-E transmission or DTC P0973, P0976, P0979, or P2764 for the 5L40-E/5L50-E transmission
Torque Converter Clutch (TCC) Pressure Control Solenoid Control Circuit High Voltage | DTC P2762, P2763, or P2764 for the 6L50/6L80/6L90 transmission
P2769 | Torque Converter Clutch (TCC) Enable Solenoid Control Circuit Low Voltage | TCM | DTC P2769 or P2770
P2770 | Torque Converter Clutch (TCC) Enable Solenoid Control Circuit High Voltage | TCM | DTC P2769 or P2770
P3400 | Cylinder Deactivation System Performance | ECM | DTC P3400
P3401 | Cylinder 1 Deactivation Solenoid Control Circuit | ECM | DTC P3401, P3425, P3441, or P3449
P3425 | Cylinder 4 Deactivation Solenoid Control Circuit | ECM | DTC P3401, P3425, P3441, or P3449
P3441 | Cylinder 6 Deactivation Solenoid Control Circuit | ECM | DTC P3401, P3425, P3441, or P3449
P3449 | Cylinder 7 Deactivation Solenoid Control Circuit | ECM | DTC P3401, P3425, P3441, or P3449
U0073 | High Speed Communication Bus | -- | DTC U0073
U0101 - U0249 | CAN-Bus No Communication with XXX Control Module | -- | DTC U0100-U0249
U1401 | Lost Communications Between AD and ADG | NIM | DTC U1401
U1814 | Powertrain High Speed Communication Enable Circuit | ECM | DTC U1814
U2099 | High Speed Communication Enable Circuit | BCM | DTC U2099
U2100 | CAN-Bus Circuit Malfunction | -- | DTC U2100
U2121 | No Communication with Radio Display | Radio | DTC U2121